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Oak Tree House, Alan Farnaby Way, Sheriff Hutton Industrial Park,
York Road, Sheriff Hutton, York, YO60 6PG
Tel: 01347 878972●E-Mail: info@whlgroup.net●www.whlbuildingservices.co.uk
CONTRACT NAME:			Portwest Clothing
CONTRACT No.			C2206
QUOTE REF No.			Q008
ESTIMATE No.			E21047
SITE ADDRESS:			Fields End Business Park, Thurnscoe S63 0JF

MAIN CONTRACTOR:		Simpson York Ltd
Contract Manager:			Mark Cregan
QS:					James Fuller

STEEL CONTRACTOR:		Gravica
Contact:				Daniel Cox
ARCHITECT:				WHP Architecture
Contact:				Tom Edwards

Contract Deed:		Yes		Period		12 Years
SITE TREATED AS: 			INLAND
THE BELOW SPECIFICATION IS TO BE READ IN CONJUNCTION WITH: Q008
ROOF TYPE: COMPOSITE
EXTERNAL SHEET PROFILE:			RW
EXTERNAL GAUGE:				0.5mm
EXTERNAL COLOUR:				Goosewing Grey
EXTERNAL COATING / GUARANTEE:	XL Forte
LINER PROFILE:				Lightly planked
LINER GAUGE:				0.4mm
LINER COATING:				Cleansafe 15
CORE THICKNESS:				100mm
CORE TYPE:					Quadcore
COMPOSITE MANUFACTURER:		Kingspan
ROOF U VALUE:				0.18 W/m²K

ROOFLIGHTS
ROOFLIGHT TYPE:   				FAIRS
ROOFLIGHT %:				10%
OUTER ROOFLIGHT:				3.0kg
INTERMEDIATE:				10mm Polycarbonate
INNER ROOFLIGHT:				1.5kg
ROOFLIGHT U VALUE:			1.2 W/m²K
ROOFLIGHT L VALUE:			36%
ROOFLIGHT G VALUE:			36%
ROOFLIGHTS FRAGILITY:			25 Years non fragility
MANUFACTURER:				Hambleside Danelaw






ROOF FIXINGS AND FLASHINGS
TO MATCH CLADDING (Y/N):		Yes
FLASHING COLOUR:				Goosewing Grey
FLASHING COATING / GUARANTEE:	XL Forte
FIXINGS / GARANTEE:			Stainless Steel / 25 Years
SEALANTS / GUARANTEE:			Enhanced / 25 Years

GUTTERS
GUTTER TYPE:				Trimline external
MATERIAL:					0.7mm pre-coat steel
COLOUR:					Goosewing Grey
COATING:					HPS200 Ultra

DRAINAGE SYSTEM
SIZE:						150mm x 150mm
MATERIAL:					0.7mm pre-coat steel
COLOUR:					Goosewing Grey
COATING:					HPS200 Ultra
QUANTITY:					To suit gutter calculations
LOCATION:					To suit gutter calculations









COMPOSITE WALL CONSTRUCTION (HIGH LEVEL)
EXTERNAL SHEET PROFILE:			Trisomet	
ORIENTATION:				Vertical
MODULE WIDTH(S): 			1000mm
EXTERNAL GAUGE:				0.5mm
EXTERNAL COLOUR:				Goosewing Grey
EXTERNAL COATING/GUARANTEE:	HPS200 Ultra / 40 Years
LINER PROFILE:				Lightly planked
LINER GAUGE:				0.4mm
LINER COATING:				PE15
CORE THICKNESS:				80mm
COMPOSITE MANUFACTURER:		Tata
U VALUE:					0.25 W/m²K		

COMPOSITE WALL CONSTRUCTION (‘PICTURE FRAME AREAS’)
EXTERNAL SHEET PROFILE:			Trisomet	
ORIENTATION:				Vertical
MODULE WIDTH(S): 			1000mm
EXTERNAL GAUGE:				0.5mm
EXTERNAL COLOUR:				Albatross / Merlin Grey
EXTERNAL COATING/GUARANTEE:	HPS200 Ultra / 40 Years
LINER PROFILE:				Lightly planked
LINER GAUGE:				0.4mm
LINER COATING:				PE15
CORE THICKNESS:				90mm
COMPOSITE MANUFACTURER:		Tata
U VALUE:					0.25 W/m²K	


WALL FIXINGS AND FLASHINGS
TO MATCH CLADDING (Y/N):		Yes
FLASHING COATING:			HPS200 Ultra
FLASHING COLOUR:				To match the adjacent cladding
FIXINGS / GUARANTEE:			Stainless Steel / 25 Years
SEALANTS / GUARANTEE:			Enhanced / 25 Years

OPENING INSULATION
GOODS DOORS:				75mm
PERSONNEL DOORS:			25mm
WINDOWS:					25mm
INSULATION TYPE:				PIR

TECHNICAL
FIREWALL GRID LINES:			GL J1-19 and J19 - E19 
FIREWALL SPEC:				60 minutes
AIR TIGHTNESS TO BE ACHIEVED: 	5.0 m³/ (h.m²) at 50 Pa.
GUTTER CALCULATIONS: 			Based on 1 year return period

OTHER
ROOF PENETRATIONS:			N/A
SHELF ANGLE:				N/A
LOUVRE TYPE:				N/A

PLEASE SIGN AND DATE BELOW TO CONFIRM THE ABOVE SPECIFICATION IS SATISFACTORY:
SIGNED BY: _________________________________________________________________
COMPANY: _________________________________________________________________
DATE: _______________________
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