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Alma Public House Demolition Plan / Access statement


				
				Worksite: The Alma P/H, Wombwell, Barnsley 
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A COPY OF THIS DOCUMENT MUST BE PRESENT ON SITE 
AND A FULL DOCUMENTATRY BRIEFING UNDERTAKEN TO ALL ON SITE PERSONNEL, SUB-CONTRACTORS AND VISITORS 
BEFORE ANY CONSTRUCTION ACTIVITY COMMENCES






	

	Name, Title
	Signature
	Date

	Prepared by
	Anthony Lidster.
	
	28.5.2019




Construction Method Statement

	1. Contract Company:
	2. Order Number

	Dove Retail Ltd.

	

	
	

	3. Exact location of the Work:

	The Alma P.H , Alma street, Wombwell , Barnsley , S73 0DE


	4. Work to be Undertaken:

	 
Demolition and clearance of public house The Alma PH.

	5. Duration of Work
	Anticipated start date
	 Anticipated end date

	 20 working days 

	 T.B.C


	



	6. Completion Criteria – States how the worksite will be left

	Daily 
	Upon Completion of Works
	Handover Arrangements

	To sign in and out of site with the Site Supervisor


	Site cleared to customer satisfaction


	Inform customer upon completion 




	

Access And Egress continued over page……

















7. Access & Egress - To and from the normal place of work. This MUST be specific as all other areas become prohibited.


	 
Access into the site from the B6096 Hough Lane/ Church St onto summer lane then onto alma street and access into site parking area / welfare facility.

Temporary Hera’s fencing erected to the front boundary of the public house site. The other 3 boundaries have suitable fencing in place.

Access in to the parking area and welfare site to be fenced with heras type fencing. Accessed through a temporary gate.

Traffic will be managed into site with an appointed banks man.

Road sweeper on standby.
[image: C:\Users\costco118\Desktop\Alma PH site access route.JPG]

	

	






8. Assembly Point - Not Ambulance Meeting Point. Indicate egress to the Assembly Point in the event of an emergency.

	
Welfare cabin opposite in the car park.

[image: C:\Users\costco118\Desktop\Alma PH site location Plan.JPG]

	

	

	

	9. Emergency Contact: (24 hour): Name    Harvey Lidster                         Tel No 07767 880802

	10. First Aid Arrangements:  First Aid Kits and Eye Wash Bottles available on site

	11. Welfare – welfare cabins provided , portable toilet

	12. Accident/Incident Reporting: All accidents and Incidents must be reported to Lidsters Main Office as soon as possible.  


	

13. Technical Content of Work

	1. Confirmation from client that all services disconnected / isolated.
2. Prior to establishment of site all Asbestos, identified by type 3 survey to be removed.
3. Hand demolition to gable (see attached drawing plan).
4. Buildings demolished by way of 360 Excavator with grab attachment. Building demolished in phases under banks man supervision.
5. Dust boss suppression system available.
6. Materials separated mechanically by 360 excavator with waste handler.
7. Material loaded into 8 wheel tipping wagons / roll on off skips and sent to licenced tipping facility.
8. Building removed to ground level and left free from rubbish.
9. Site left level and tidy in line with specification.
NB – Detailed Demolition Plan in Appendix B 

	14. Site Specific Risks
	
	
	Risk Assessment 

	
	YES
	NO
	Hazard
	Risk
	Control Measures

	Gas




	Y




	
	Presence of Domestic Gas



	Explosion




	Confirmation of supply being disconnected to be notified by Customer prior to work commencing


	Electricity






	Y






	
	Live current






	Electrocution
Explosion
Fire




	Electric supply to be isolated and retained for the duration of the new build.

 



	Water

	Y

	
	Supply interruption

	Flooding Waste
	To be retained for new build 


	Movement of Plant & Machinery
	Y

	
	Man / Machine Interface
	Strike with Machine
	Banks man appointed


	Effects of Work on Public Areas

	Y


	
	Moving Plant & Machinery
 Noise, Dust
	Contact, Strike, Pollution
	Worksite access point to be locked off preventing access when site
 
Unattended. Signs and notices to be posted

	Traffic Management


	Y


	
	Public Interface 
Mud on road

	Nuisance
Collision

	Banks man appointed
Sweeper to be used as needed


	Waste Disposal


	Y


	
	Waste material 


	Pollution
Contamination

	Appropriate disposal arrangements to licensed tip 


	Working at Height




	Y




	
	Person falling
Falling objects



	Death, Serious Injury



	All work at heights to be undertaken from scaffold platform fitted with hand rails and toe boards or from Mobile Elevated Working Platform

	

Generic Hazards and associated Risks Assessed included at Appendix A

	
USING PLANT AND EQUIPMENT


	EXCAVATOR 360	15

	HAND TOOLS (none electrical)	17

		

	

	LOADING/UNLOADING LOW LOADER                                                                                 22 B

	
SPECIALIST TASKS


	DEMOLITION (soft strip)	23

	DEMOLITION (structural)	24

	GENERAL


	FIRE PRECAUTIONS (site in general)	26

	PROTECTION OF PUBLIC/OPERATIVES (on site)	29

	SITE MOBILE PLANT/TRAFFIC (general)	30

	UNDERGROUND SERVICES	31

	WORKING AT HEIGHT	32

	REMOVAL FIBRE CEMENT ROOF SHEETS                                                                               AD32A

	

	REMOVAL STEEL STRUCTURE                                                                                         AD32C














	15. Plant / Equipment:

	To be used
	Details
	 Competent Operator

	360 20 tonne Excavator grab. attachment
	
	CITB competent

	8 wheeled tipper lorry
	
	HGV Driving Licence

	Mobile elevating platform
	
	Competent operative

	
	
	

	
	
	

	16. Personal Protective Equipment to be used:

	Hard Hats
	 
Yes – Mandatory

	Safety Footwear
	Yes -  Mandatory

	Hi-visibility vest
	Yes – Mandatory

	Ear Defenders
	Yes – Mandatory where signs fitted

	Gloves
	Yes – As dictated by PPE/Task assessment

	Safety Glasses
	Yes – As dictated by PPE/Task assessment

	17. Hazardous Substances:

	COSHH Assessments will be available on site for the following hazardous substances:

	 Diesel 

	 Oil 

	 Petrol 

	18. Subcontractors to be used:
	 All must be approved by Lidsters and have their own Method Statement

	Asbestos Removal Contractors. 



	

	

	19. Environmental Protection Arrangements

	 Hazard
	Risk
	Control

	Noise & Vibration
	Disturbance to residence
	Noise to be kept to a minimum

	Lighting
	None
	Day shifts only

	Traffic Disruption
	To local residents & business
	One way traffic system in place

	Pollution
	Emissions from Plant
	Engines to be switched off when not in use

	Landscape
	Disturbed ground
	To be levelled upon completion

	Waste
	Inadequate disposal
	Disposed of to licensed tip

	Protected Species
	None 
	

	Archaeology
	None
	

	Tree Preservation Orders
	None
	






Method Statement Briefing Form



	Location of Brief
	


	Name of Briefer
	


	Signature of Briefer
	



		

To ensure that EJ Lidster Construction are able to maintain auditable records of attendance of safety briefings you are required to sign below as proof of attendance and understanding of details briefed.


	Name
	Date
	Depot / Site
	Signature

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	







APPENDIX A: GENERIC RISK ASSESSMENTS


GENERIC RISK ASSESSMENT INDEX


	WORK ACTIVITY	REF


	
USING PLANT AND EQUIPMENT


	EXCAVATOR 360	15

	HAND TOOLS (none electrical)	17

	MEP's (Mobile Elevated Platforms)	20

	

	LOADING/UNLOADING LOW LOADER                                                                                 22 B

	
SPECIALIST TASKS


	DEMOLITION (soft strip)	23

	DEMOLITION (structural)	24

	GENERAL


	FIRE PRECAUTIONS (site in general)	26

	PROTECTION OF PUBLIC/OPERATIVES (on site)	29

	SITE MOBILE PLANT/TRAFFIC (general)	30

	UNDERGROUND SERVICES	31

	WORKING AT HEIGHT	32




 E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 15

	ACTIVITY

EXCAVATOR (360 tracked)

	HAZARDS

Ground conditions, poorly maintained, to feet, head, hands, overloading overhead electric cables, underground services, to third parties/pedestrians in vicinity of operations, collapse of boom, refuelling (COSHH).

	PEOPLE EXPOSED

Operator and anyone on site.

	ACTION/CONTROLS TO REDUCE RISK

Only trained and competent drivers to operate machine (CITB licence holder or similar).
Machine to be maintained in good repair including the correct retaining clips fitted to buckets and safety devices fitted and working on quick release buckets.
Mirrors to be fitted around machine including to rear to aid all round vision.
Not to be operated within the vicinity of overhead cables.
Operator to be warned of services not to dig within 500mm of underground services.
Weekly inspection of machine to be carried out and results logged.
Care to be taken when working in the vicinity of excavations.
To be guided by banksman in tight areas.
Safe working load (SWL) to be marked on machine, not to be exceeded.
Check valves to be fitted.
Lifting gear only to be attached to tested lifting eyes.





	PERSONAL PROTECTIVE EQUIPMENT

Safety boots and high viz vest/jacket, helmet to be worn outside machine, gloves to be used for refuelling.

	TRAINING

Operator to hold CITB licence or similar, and advised of COSHH requirements for diesel.

	ASSESSMENT REVIEW

To be reviewed from time to time.




 E J LIDSTER SALES  LTD
GENERAL RISK ASSESSMENT

REF 17

	ACTIVITY

HAND TOOLS (none electrical)

	HAZARDS

Flying particles, electric shock to hands, feet, eyes and/or body.

	PEOPLE EXPOSED

Operative primarily.

	ACTION/CONTROLS TO REDUCE RISK

Tools provided must be in good repair, be maintained in good repair and be suitable for the purpose for which they are to be used.
Eye protection to be provided and used when working with cold chisels, manual drills or other tools where there is a risk of flying particles or pieces of tool breaking off.
Open bladed knives, screwdrivers and other sharp tools to be carried and used so as not to cause injury to the user or others.
Non ferrous (spark free) tools are to be used in flammable atmospheres.
Insulated tools must be used where there is a possibility of live electrical work.
Tools to be regularly checked to ensure they remain in good condition.







	PERSONAL PROTECTIVE EQUIPMENT

Helmets and safety boots to be worn, gloves may be necessary and as per site rules.

	TRAINING

All operatives to be instructed in the correct method of use and maintenance requirements.

	ASSESSMENT REVIEW

To be reviewed from time to time and revised as necessary.




E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 20

	ACTIVITY

MOBILE ELEVATED PLATFORMS (MEP) (using)

	HAZARDS

Overturning, fall from platform, fall of materials, electric shock.

	PEOPLE EXPOSED

Operator and people in and around.

	ACTION/CONTROLS TO REDUCE RISK

Only to be operated by a trained and competent person holding relevant certificate of training/competence.
Platform must be maintained in good repair at all times/to be inspected daily before use.
Ensure no overhead lines are present in work area.
Ensure the wind speed is not excessive.
Ground conditions must be suitable and stable and where necessary outriggers and stabilisers must be safely deployed.
Safe working load not to be exceeded.
Signs and barriers to be erected to prevent access under the working area.
Work to be carried out within the specified reach of the unit used.
All tools and equipment to be secure from falling.
Operatives not to overstretch/reach from platform.




	PERSONAL PROTECTIVE EQUIPMENT

As per site rules, safety helmets and safety boots to be worn.  In most cases harnesses to be worn by all using platform.

	TRAINING

Only trained operatives to use Mobile Elevated Platforms.

	ASSESSMENT REVIEW

To be reviewed on site to ensure assessment covers all site conditions. 




 
E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 22 B 

	ACTIVITY

PLANT: loading/unloading hiab lorry – lifting

	HAZARDS

Uneven/soft ground conditions, adverse weather, overhead cables, untrained operatives, poorly maintained machines, overloading, communication problems, materials falling, collapse/failure of crane, incorrect capacity of crane

	PEOPLE EXPOSED

Operative and anyone in the vicinity of operations.

	ACTION/CONTROLS TO REDUCE RISK

Machine selected by competent operator
Emergency evacuation procedure/rescue procedure in place
Operator/slinger to maintain position of safety at all times – out with the reach of the load
Only tested lifting gear to be used
Test/inspection documents to be checked to ensure they are up to date
Ground/base to be suitable for stability of crane- avoiding services/manholes
Lifting plant to be provided
Work within the Safe Working Loads of the equipment
Load to be positioned and strapped onto lorry before lifting chains removed 
Only trained banksman/slinger to attach loads
Adequate visibility/signalling arrangements to be made
Third parties controlled/kept out of area





	PERSONAL PROTECTIVE EQUIPMENT

Helmets, hi-visibility vests and safety boots to be worn by all operatives in the vicinity of operations, gloves may be necessary for slinger, eye protection where necessary

	TRAINING

Banksman/slinger and crane operator to be trained and competent and advised of any site hazards e.g. overhead services

	ASSESSMENT REVIEW

To be reviewed by Operator at each location prior to load/unload 




 E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 23

	ACTIVITY

DEMOLITION: Soft, non-structural, partitions, ceilings, cladding, plaster etc.

	HAZARDS

Site activity and conditions, access, dust, services, manual handling, noise, head, feet, electric shock, vibration.  (If asbestos found separate assessment to be carried out).

	PEOPLE EXPOSED

Operatives primarily, persons in the vicinity.

	ACTION/CONTROLS TO REDUCE RISK

Survey to be carried out before any work undertaken to ensure services are identified and cut off/isolated, that walls etc., to be removed are non-structural and to ensure there is no asbestos present.
Work plan/method statement required before work starts.
Waste to be removed with the use of mechanical aids whenever possible (chutes, trolleys, hoists etc).
Only 110v electrical tools to be used.
Tools to be carefully selected to reduce noise, vibration etc.
Platforms/access to comply with same requirements as on construction job.
Work area to be sectioned off to prevent persons not carrying out work from gaining access to work area.




	PERSONAL PROTECTIVE EQUIPMENT

Helmets and safety boots to be worn at all times, ear protection, dust masks, goggles, gloves to be provided as outlined in method statement.

	TRAINING

All operatives to receive training in good working practices as outlined in method statement.  Kinetic handling training may be required.

	ASSESSMENT REVIEW

Assessment to be reviewed before any work of this nature takes place.




E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 24

	ACTIVITY

DEMOLITION of structures.

	HAZARDS

Site activity and conditions, access, collapse of structures, dust, exposure to services, manual handling, noise, vibration, machinery, structure stability (pre-stressed concrete) head and feet.

	PEOPLE EXPOSED

Operatives and people in vicinity including adjacent premises.

	ACTION/CONTROLS TO REDUCE RISK

On site survey to be undertaken to enable an accurate understanding past features and present condition prior to any demolition, characterising type of structure, condition, need for temporary support, confined spaces, overhead services, hazards such as asbestos, lead paint or steelwork or other toxic residues.
Protection of public, site enclose/fence off, danger notices to display, provision of banks man to exclude passers-by away from potential danger areas when working near boundaries.  Exclusion zones to be discussed and set to prevent danger.
Minimise working at heights, consider means of access, equipment, pre-weakening of structure. 
Removal of services, method for dealing with toxic/flammable residues, waste transport and disposal, safety co-ordination.
Minimise noise by selection of plant and equipment.
Only to be undertaken by competent contractor.  (To be checked out at tender stage).
Method statement must be drafted and checked before work starts.



	PERSONAL PROTECTIVE EQUIPMENT

Helmets and safety boots must be worn at all times.  Dust masks may be required, gloves and ear defenders.  Safety harnesses may be required in certain instances.  If lead or asbestos present, specific risk assessment required to decide on requirements.

	TRAINING

Supervisors must be trained and competent to carry out demolition work.  Operatives to receive training in good working practices and kinetic handling.

	ASSESSMENT REVIEW

To be reviewed prior to all demolition work and revised where necessary.




 E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 26

	ACTIVITY

General site activities "FIRE"

	HAZARDS

Fire, smoke.

	PEOPLE EXPOSED

Operatives and visitors to site, may include occupants of partially completed flats/houses.

	ACTION/CONTROLS TO REDUCE RISK

Firefighting equipment to be available on all sites for:
a)	Accommodation on site.
b)	Hot work being carried out.
c)	Inside multi storey blocks of flats.
Alarm system to be established on multi storey blocks of flats.  Manual bell/air horn or similar.
Smoke alarms to be fitted to welfare cabins.
Procedure to be established for raising alarm and posted out on site.
Operatives, visitors to be advised of assembly point location.
Extra precautions to be taken during works in partially occupied flats e.g. no smoking, double checks after hot work etc.
Permit to work system to be established for hot works.
Fire escape routes to be provided in flats during construction and marked as such.
Flammable materials not to be allowed to accumulate (tidy up regularly as work progresses).




	PERSONAL PROTECTIVE EQUIPMENT

As per site rules.

	TRAINING

All operatives on site to be advised of site rules, position of fire extinguishers, assembly point and instructed as to what the fire warning system is. 

	ASSESSMENT REVIEW

To be reviewed from site to site. 




E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 29

	ACTIVITY

PROTECTION OF PUBLIC/OPERATIVES (on site)

	HAZARDS

Site activities, plant, access to scaffolds, under scaffolds, stored materials, excavations, open manholes, BT boxes etc.

	PEOPLE EXPOSED

Operatives, general public and children.

	ACTION/CONTROLS TO REDUCE RISK

Permanent perimeter fencing to be installed at an early stage.
Construction area to be fenced off with heras fencing to protect public as necessary, work adjacent to boundaries to be checked for potential dangers to the public, banks man provided as necessary to exclude pedestrians from danger areas.
Signs to be erected on fencing i.e. Danger, Keep Out. 
Signing in procedure and induction training to be carried out on all sites.
Excavations to be fenced off or fully back filled.
Incomplete scaffold signs to be displayed where necessary.
Ladders to be removed from scaffolds at end of shift.
Manholes, BT boxes etc., to be securely covered at all times.
Materials to be safely stacked.
Sites to be kept in good order.
Security guards to be considered.
Contact local schools.




	PERSONAL PROTECTIVE EQUIPMENT

Safety boots/shoes, high viz vests/jackets and helmets to be worn by all entering the build area.

	TRAINING

All operatives to receive induction training.

	ASSESSMENT REVIEW

To be reviewed from site to site.






E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 30

	ACTIVITY

SITE TRANSPORT

	HAZARDS

Injury to persons on site

	PEOPLE EXPOSED

Site operatives, general public, children

	ACTION/CONTROLS TO REDUCE RISK

Traffic management plan to be set up and displayed on site.
Pedestrians to be protected from plant and equipment.
Compound to be set up to keep vehicles and pedestrian routes separate.
Separate access to be provided to compound for pedestrians.
One way system to be established wherever possible.
Speed humps to be considered.
Speed of vehicles to be restricted (signs).
Plant warning signs to display.
Reversing delivery vehicles to be guided by banks man.
F/lifts and mobile plant to be fitted with reversing warning systems.
Plant to be effectively immobilised at the end of shift, lock machine where possible.
Remove keys when machine left unattended.
All excavators and f/lifts to be fitted with sufficient rear view mirrors, kept in good repair, to aid reversing manoeuvres.
Where mirrors are not deemed to be sufficient then plant must be fitted with a rear view camera e.g. large dump trucks.
Windscreens, side screens and rear screens to be regularly cleaned to allow for good vision.



	PERSONAL PROTECTIVE EQUIPMENT

Reflective coats/waistcoats to be worn by banks men/operatives working with plant.

	TRAINING

Induction training to be carried out as necessary.

	ASSESSMENT REVIEW

To be reviewed from site to site. 






E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 31

	ACTIVITY

UNDERGROUND SERVICES (working in vicinity)

	HAZARDS

Electric shock, explosion, fire, burns.

	PEOPLE EXPOSED

Operatives carrying out works.

	ACTION/CONTROLS TO REDUCE RISK

Excavations to be placed under supervision of competent person.
Service drawing to be provided/checked before any digging on site.
Cable locator to be used to check area.
No excavators to be used within 500mm of service positions.
Operatives carrying out hand digging to be fully clothed (natural fibre clothing), to guard against burns.








	PERSONAL PROTECTIVE EQUIPMENT

Helmets, safety boots and reflective w/coats to be worn at all times.  Ear protection and goggles may be required during certain processes/activities.

	TRAINING

All operatives to be advised of known service locations.

	ASSESSMENT REVIEW

To be reviewed from site to site. 








E J LIDSTER SALES LTD
GENERAL RISK ASSESSMENT

REF 32

	ACTIVITY

Working at height

	HAZARDS

Fall of persons, materials.

	PEOPLE EXPOSED

Operatives working at height, operatives working below, members of the public.

	ACTION/CONTROLS TO REDUCE RISK

Safe means of access to the work place using ladders, scaffold, mobile towers, mobile platforms etc.
Edge protection to be provided to all openings, edges where persons may fall from height.
Harnesses to be used where edge protection is not practical.
Area below to be fenced off or banks man provided.
Signs to display (men working overhead).
Redundant materials should be cleared away without delay, but not thrown from high level (bombing).  A debris chute should be used or materials collected and lowered in suitable containers.
The fall of materials should be prevented by the use of debris netting, brick guards and fans. 





	PERSONAL PROTECTIVE EQUIPMENT

Safety boots and helmets to be worn at all times, harnesses and safety lines may be necessary in some instances.

	TRAINING

All operatives to be induction trained and advised of control measures.

	ASSESSMENT REVIEW

To be reviewed from site to site.
















            











                                 APPENDIX B: DEMOLITION PLAN


Grange Lane, Stairfoot, Barnsley 



SEQUENCE AND METHOD OF DEMOLITION IN ACCORDANCE WITH
BS 6187:2000 “CODE OF PRACTICE FOR DEMOLITION”
5.2.3 PREPERATION OF METHOD STATEMENTS



















DEMOLITION PLAN

	
STAGE
	
TASK
	
ACHIEVED

	
	
Asbestos identified in type 3 survey removed prior to demolition.
	


	
	
Confirmation that all Asbestos removed.
	

	
	Site area to be fenced with heras type fencing.
	

	
	Soft strip carried out on all internal soft furnishings carpets, timbers, door casings etc. By hand.
	

	
	Hand demolition to gable end access from mobile elevating platform. (See attached location drawing for hand demolition.) 

	

	
	Buildings to be demolished by used of 360 Excavator with mechanical grapple.
All demolition to be undertaken under Banks man supervision ensuring safe working and that all falling debris within fenced perimeter.

	

	

	Materials arising from demolition sorted by mechanical waste handler on site.
	

	
	Materials loaded in to tipper wagons. All loading to be undertaken within site perimeter. Materials taken to licensed tipping facility.
	

	

	Site to be levelled in line with specification
	

	

	Site to be cleared of all waste material
	

	

	Fencing will be retained across front of the site to prevent un wanted access and encroachment.
	

	

	
Site to be handed back to the Client upon satisfactory completion of all of the above

	












Hand demolition of structure to a safe height from mobile elevating platform. Location has been agreed with neighbouring owner, this will be achieved from within their fenced car parking area. 

See attached area plan.

[image: C:\Users\costco118\Desktop\Alma gable hand demolition.JPG]
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