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	Doncaster Road, Darfield – Stage 1 Road Safety Audit
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	Overseeing Organisation:
	Barnsley Council

	RSA Team:
	Haydn Vernals (Team Leader) & Sarah Vernals (Team Member)

	Design organisation:
	Paragon Highways







OFFICIAL

3
		OFFICIAL

1. [bookmark: _Toc236823475]ROAD SAFETY AUDIT DECISION LOG
	RSA problem
	RSA recommendation
	Design organisation response
	Overseeing Organisation response
	Agreed RSA action

	A-01 Location: Doncaster Road – At the ghost island

Summary: Drainage – Ineffective drainage of surface water may increase the risk of skidding or loss of control type collisions
	It is recommended that all areas are provided with suitable surface water drainage measures to minimise the risk of standing water and detritus
	Accepted – suitable drainage design shall be provided at detailed design stage and agreed with Barnsley Council as part of the S278 process
	
	

	A-02 Location: Doncaster Road – At the ghost island junction

Summary: Skidding Resistance – Carriageway surfacing across part lane widths may increase the risk of loss of control type collisions
	It is recommended that the widening provided is done in full lane widths and the revised crown of the road is located such to avoid the application of any adverse camber
	Accepted – the limits of the surfacing and crown position will be provided as part of the detailed design and agreed with Barnsley Council as part of the S278 process
	
	

	A-03 Location: Barnsley Road – At the eastern development access

Summary: Landscaping – Future growth from the trees and bushes may obstruct visibility consequently increasing the risk of junction related collisions
	It is recommended that junction visibility envelope is cleared of vegetation
	Accepted – the vegetation shall be removed insofar as to enable the formation of the junction and associated junction visibility in perpetuity
	
	

	A-04 Location: Barnsley Road – At the eastern development access

Summary: Specific Road Users – Lack of provision for users who rely on mobility aids may increase collisions involving this user group
	It is recommended that dropped kerbs with tactiles are provided across the development access
	Accepted – the junction will include tactile dropped crossings with further details provided at Detailed Design stage.
	
	




	A-05 Location: Barnsley Road

Summary: Pedestrians – Location of a dropped crossing may increase the risk of collisions involving pedestrians
	It is recommended that the dropped crossing is located to minimise the crossing distance whilst maintaining inter-visibility between pedestrians waiting to cross and approaching vehicles. This could be achieved by relocation of the crossing points marginally further into the side road
	Accepted – the tactile crossing point is located further into the site access and shown indicatively on amended drawing PRGN-1229-HGN-DR-CH-103C. The location of the crossing will be agreed with Barnsley Council as part of the S38 process
	
	

	A-06 Location: Doncaster Road – Between the western development access and Barnsley Road

Summary: Pedestrians – Close proximity to a higher speed road may increase the risk of collisions or injuries involving pedestrians on the footway
	It is recommended that a buffer strip is provided appropriate to the speed of the road. Some guidance on suitable widths is highlighted in LTN 1/20 Table 6.1 for cycle routes but these remain relevant to footways
	Not Accepted – the guidance relates to cycle tracks only. The proposals include a refuge island that connects to the recently constructed shared cycle facility along the north side of Doncaster Road. This contains an edge of carriageway marking providing some separation (buffer) between the carriageway and cycle facility. There are no new cycle tracks proposed on the south side of Doncaster Road.
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1. [bookmark: _Toc236823476]DESIGN ORGANISATION AND OVERSEEING ORGANISATION STATEMENTS
	Design organisation statement

	On behalf of the design organisation I certify that:
1) the RSA actions identified in response to the road safety audit problems in this road safety audit have been discussed and agreed with the Overseeing Organisation.

	Name:
	Leigh Ogden

	Signed:
	LJ Ogden

	Position:
	Director

	Organisation:
	Paragon Highways

	Date:
	04/08/2026



	Overseeing Organisation statement

	On behalf of the Overseeing Organisation I certify that:
1) the RSA actions identified in response to the road safety audit problems in this road safety audit have been discussed and agreed with the design organisation; and
2) the agreed RSA actions will be progressed.

	Name:
	Nathan Copley

	Signed:
	

	Position:
	

	Organisation:
	Barnsley Council

	Date:
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