31 Highbank, Thurlstone, S36 9QH
Summerhouse Construction Notes
Construction
Fire Escape
Form opening through existing bedroom wall and install solid core flush door and lining.
Stonework

Build up 3No. stone piers approx 300mm x 300mm extending from existing pads.

The existing soldier course of stonework is to be removed and new stonework extended up to match the existing and including stone cills under the windows.
Roof
Fibre Cement Anthracite Grey Slate roof fully clipped on 25 x 38 battens on a breathable membrane fixed to
100 x 50 treated softwood joists at 600 centres

100 x 50 bearer bolted to existing house wall with joist hangers @ 600 cts.

150 x 50 treated softwood bearer over front window, 

150 x 50 treated softwood purlin mid span supported on a 750x 75 oak post and 2no. 100 x 50 studs in the rear stud wall
100mm rockwool insulation between joists and

12mm Foilbacked plasterboard with taped and filled joints

940 x 980 PK04 Velux rooflight set high in roof.
North Wall
125 x 19 Redwood shiplap boarding on building paper on

100 x 50 Treated softwood studwork with

100mm rockwool insulation between studs and

12mm Foilbacked plasterboard with taped and filled joints
100mm high skirting board

Windows & Door

White UPVC slimline Windows to match the existing on hardwood framing with 100mm wide window boards and a 
White UPVC half glazed door and frame.
Floor

18mm WBP Plywood on

100 x 50 Treated softwood joists on d.p.c. on 38mm precast concrete pads

