
Build to include roof 
•	Clear area of all concrete and small block storage shed
•	Customer to remove concrete sectional garage  
•	Dig strip footing using hired mini digger, allowing for a dig of 900mm below Ground level*
•	Dumper or track barrow to be hired to help with spoil removal
•	Spoil to be removed via grab wagon if the spoil can be piled, if not skips will be used
•	Once checked by building control, mass fill footing with concrete, approx. 6m3 of concrete needed
•	Concrete pump to be hired if needed
•	Drains to be altered if needed to accept new rain water pipe 
•	Build extension as agreed with client and supplied drawings, approx. 2300mm x 6633mm x 4280. Bricks to be confirmed but have been priced up on Carlton Weathered Red
•	Squint bricks to be cut and bonded together to achieve the correct degree so brickwork can run on an angle 
•	Stone heads and cills supplied and fitted if needed
•	New floor is to be hard cored, DPM laid and concreted in accordance with building regulations  
•	Concrete pump will be hired if needed
•	All walls, floor space, and roof space to be insulated in accordance to building control and supplied drawings
•	Timber floor joists to be built in at first floor level and chipboard flooring to be laid 
•	Traditional hip timber roof to be built to as shown on supplied drawings
•	A structural engineer will advise on the correct way to support the existing roof and his fee is included in the costings 
•	Roof to be felted, lathed and reclaimed slates to be supplied and laid to match existing roof
•	Install fascia, soffit and gutter to match existing
•	Once water tight, existing house wall to be removed to allow doorways in to extension at ground floor and first floor level where shown on plans
•	All lintels needed to be supplied and fitted
•	Scaffold to be erected at each necessary stage of the job

•	All the required materials and labour involved with the above build are included in the above price. Concrete, steel, structural engineer, skips, plant machinery (mini diggers & whacker plate), scaffolding are all included in the above price. Also, removal of all debris and unwanted materials at the end of the job

* When the footing has been dug to the required depth, building control will come out and either allow us to pour concrete, or ask us to dig down deeper. If we are asked to dig deeper, this may incur additional cost

Plastering 
•	All extension to be dry lined and skimmed
•	All RSJ’s to be fire lined in accordance with building regulations
•	Any walls / ceilings in the existing house affected due to the building works to be made good
•	Stud walls to be insulated, dry lined and skimmed

Electrics     
•	No electrics included

Joinery 
•	Skirting boards to match existing to be supplied and fitted
•	Door / casings to be supplied and fitted (6 panel doors) where shown on plans
•	Architrave to match existing to be supplied and fitted 
•	Stud walls to be erected on first floor to divide the living space where shown on plans 
•	Window boards to be supplied and fitted

Plumbing 
•	No plumbing included



Windows 
•	Two windows to be supplied and fitted to match existing house windows in extension
•	These will comply\ with building control with the necessary fire escapes etc
•	Existing bedroom window to be removed, reduced in size with brickwork and new window fitted 
[bookmark: _GoBack]•	New composite door to be supplied and fitted with sidelight window.
