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1.  NATURE OF PROJECT  
Client:



Barnsley Metropolitan Borough Council 
Address:


Town Hall




Barnsley




S70 2TA
Tel:



01226 773033
Contact:                                          Sara Scholes 
Email:
                                           SaraScholes@barnsley.gov.uk
ARCHITECTURE & LEAD DESIGNER
Address:


Property Services  




Barnsley Metropolitan Borough Council




Town Hall





Barnsley





S70 2TA
Contact:

              Ben Taylor 
Tel:



07919 917 706
Email:



bentaylor@barnsley.gov.uk
PRINCIPAL DESIGNER
Address:


Property Services  





Barnsley Metropolitan Borough Council





Town Hall





Barnsley





S70 2TA


Contact:


Ben Taylor 
MECHANICAL & ELECTRICAL ENGINEERS 

Address:


Property Services  





Barnsley Metropolitan Borough Council





Town Hall





Barnsley





S70 2TA
Contact:


Mechanical Contact – Tony Hughes 





Electrical Contact – Paul Durkin 
STRUCTURAL ENGINEER 

Address:


Design IT Structural Solutions 





37 Hall Bank,





Barnsley 





S75 1EX

Contact:


Ian Thorpe 

CIVIL ENGINEER

Address:


Shaun Tonge Engineering Ltd 

Contact:


Shaun Tonge 
PRINCIPAL CONTRACTOR
Address:


O & P Construction Services Limited





Common Lane





Wath upon Dearne





Rotherham

S63 7DX

Contracts Director: 

Andy Marshall
Tel:



07973 525889
E-mail:



andy.marshall@opconstruction.co.uk
Site Manager:


Richard Shepherd 


Tel:



07852 400815 
Email:



richard.shepherd@opconstruction.co.uk



HEALTH AND SAFETY EXECUTIVE
Address:


H.S.E.





Foundry House





3 Millsands





Riverside Exchange





Sheffield S3 8NH

Tel:



0114 291 2300

Description of Work

Construction of seven new bungalows as follows:- 


6 Nr 2 bed semi detached bungalows 



1 Nr 3 bed detached bungalow

The works also include the drainage, external works and ancillary works.

Site Address

 
Address:


Laithes Lane





Athersley 





Barnsley 





S71 3AN
Programme of Works

Commencement date

Monday 22nd November 2021
Completion date 

Friday 15th July 2022
Duration


34 weeks 
Health and Safety Objectives

a) To ensure the health, safety and welfare of all employees and all other persons on site and within the premises for which the company is responsible.

b) All work carried out by employees of the company shall be undertaken so as to ensure that the health and safety of the occupants of the building and the general public is not put at risk.
Arrangement for Managing Health and Safety

Mr D. Sutcliffe takes overall responsibility for safety measures within the company and for compliance with the Health and Safety Policy.  The Site Supervisor will be responsible for day-to-day Safety matters.

A copy of the Safety Plan will be kept on site and all personnel made aware of it.  All site personnel will be encouraged to give their views of Health and Safety to the Site Manager.

Client to brief their staff on the works and others as appropriate regarding the Safety Plan and planned construction works to ensure they are aware of construction activities and that this area is out of bound’s 
Standard Setting

Work will be carried out in accordance with the Health and Safety at Work, etc. Act 1974, the Construction (Design and Management) Regulations 2015 and all other relevant Regulations relating to Health and Safety at Work.  In addition, any specific standards dictated by the client will be satisfied.
Information for Contractors

All contractors working on the project are to be informed about any risks involved and all the Site Safety Rules.  This will be achieved by providing all contractors with a copy of the Construction Phase Health and Safety Plan and by discussions with each sub-contractor.

Project Control

A programme will be prepared to ensure work is carried out in a logical manner.  The programme will be updated weekly.

The project will be controlled by the Contracts Manager who will be communicating with the foremen of all sub-contractors.  The Manager will monitor the Health and Safety Plan.  
Contact: 
Contracts Director:
Andy Marshall

Mobile 07973 525889


Site Manager:

Richard Shepherd 
Mobile 
07852 400815
OUT OF HOURS
Andy Marshall

07973 525889 
          
Richard Shepherd 
07852 400815
Emergency Procedures

In the case of any emergency call 999 and request the appropriate emergency service.
The nearest hospital with an accident and emergency department is located within 3.2 miles as follows: 

Barnsley Hospital 
Gawber Road 
Barnsley 
South Yorkshire 

S75 2EP
Tel: 01226 730000
When developing their emergency procedures, the Principal Contractor must ensure that suitable rescue procedures are in place for when working at height is being carried out. The emergency means of escape shall be identified in the fire plan as detailed above.
STATUTORY AUTHORITIES

GAS
Name:



National Grid
Tel:



0800 001 4340
ELECTRICITY

Name:



Northern Power Grid 
Tel:



0800 375675
WATER

Name:



Yorkshire Water
Tel:



0800 573553
TELEPHONES
Name:



British Telecom
Tel:



100

ENVIRONMENT AGENCY

Name:



Environment Agency

Tel:



0800 807 060 

Induction Certificates

All employees will be briefed as to the contents of the Construction Phase Health and Safety prior to their commencement on site and signed “Induction Certificates” obtained confirming that they have been briefed.

In respect of sub-contractors, a manager or supervisor representing sub-contractor will be briefed and they will be instructed to obtain Induction Certificate off their operatives.

All operatives have been trained in the general rules of safety.

Selection Procedures

Only contractors who have worked for the company previously and have performed satisfactorily will be used on the project.  If not, they will be forced to submit their Safety Policy for approval.

Only items of plant, machinery and materials which are appropriate for the task will be used, all of which will be operated/used by skilled operatives.

When plant or equipment is hired, certificates of fitness will be obtained.  Likewise, operatives will be checked for competence and C.I.T.B. certification.
2. THE EXISTING ENVIRONMENT
The proposed site is located off Laithes Lane and Laithes Close in the predominantly residential part of Athersley, Barnsley.  The site is located on a relatively small grass peninsula, which has roads to its Northern, Eastern and Southern Boundaries, with further residential properties along the Western boundary.

Local amenities such as shops, takeaways and schools are all located relatively close to the site.  There are bus routes close by, which provide access to and from the town centre along with other local suburbs and villages. 
Access

Access will be off Laithes Lane and Laithes Close as shown on the site layout plan attached.
Traffic warning signs to be erected both sides of the entrances.

Maintenance of Access

Access must be maintained at all times to ensure safe passage of fire appliances, refuse vehicles, police and ambulance services.
Existing Drainage

Existing drainage will be protected.

Site Security

All operatives and sub-contractors will wear workwear with the Company logo. The site manager will monitor all operatives’ activities on site.
Photograph ID badges will be worn at all times
The site will be left secure at the end of each working day by securing the heras fencing with padlocks and chains to entry areas. The remaining panels are double clipped from the inside.
3. EXISTING DRAWINGS

The topographical drawings will be kept on site.

Copies of the statutory authority mains drawings will be kept on site, showing the expected position of existing mains and services.

Investigations including CAT Scanning will be carried out prior to commencement to locate existing services and drawings will be kept on site showing services affecting the proposed works.  

4. THE DESIGN

The bungalows are to be constructed as follows:- 

a) Concrete trench fill
b) Beam and block ground floor with screed on insulation

c) Brick and block cavity walls 

d) UPVC windows and composite external doors
e) Trussed roof with tile roof covering

5. CONSTRUCTION MATERIALS

All hazardous materials will be used in accordance with manufacturer’s instructions and will be disposed off in the prescribed manner.

All hazardous materials will be kept in a locked secure location separate to the welfare facilities and separate to the newly constructed bungalows.

COSHH Regulations

COSHH Assessments will be provided for all appropriate materials and kept on site.
6. SITE WIDE ELEMENTS
COVID-19 OUTBREAK (CORONAVIRUS) PRECAUTIONS

We have produced a suite of documents to deal with the hazards and health risks associated with Covid-19 as below.

1. COVID-19 Company Policy

2. Our Standard RAM’s which are referred to and revised to be site specific for each site

3. Self-Assessment questionnaire to be completed by all attending site 

4. Letter to subcontractors advising of COVID-19 measures to be implemented on all O&P sites 

5. O&P Authorised travel statement for operatives travelling to and from site

6. Construction Leadership Council, Site Operating Procedures – Version 7 dated 07.01.21 (or subsequent revisions) 

7. Site specific RAMS for COVID-19 precautions operating on site this site 

These will be appended to the rear of this construction phase plan.
It is important that these documents are referred to in relation to the various sections of this CPP

COVID-19 events are now RIDDOR reportable.
Risk Assessments and Method Statements

A Risk Assessment and Method Statement will be produced one week prior to commencing the relevant work for the following: -

a) Roof truss installation
b) Installation of beam and block ground floor

c) Stability of structures whilst carrying out construction work including any temporary structures

d) Prevention of falls

e) Installation of steel

f) Sewer connections

g) Working in close proximity to existing gas, electric and telecom services

h) Working outside site boundaries

i) Dust suppression on site

j) Movement of materials from compound to site 

k) Potential presence of asbestos cement in excavation

l) Passive Fire Protection

This list is not exhaustive and there will be additional RAMS as required.

Scaffolding

Scaffolding will be provided for all high level work internally and externally and will comply with all relevant standards by a CISRS or similar trained scaffolder. Handover certificates are to be provided following completion/alteration of scaffold. Weekly scaffold checks will be overseen by an SSSTS trained, competent working foreman.
Hypodermic Syringes, Needles and Solvents
It is likely it is possible that the proposed site for the compound and surrounding area may have been used for illicit drug use and or solvent abuse.  If needles are found, protective clothing and gloves must be worn whilst operatives are disposing of the above material.  All such materials must be disposed of in a proper manner.  If there is a possibility of syringes in the grass or overgrowth, then a rake should be used to expose them. 

Below Ground Services

All work on or adjacent to underground services shall be carried out in accordance with current legislation and the HSE guidance notes.

On completion of the various alterations and extensions to the below ground services, the exact location of the services (new and existing) will be annotated on the contract ‘As Built’ drawings, for inclusion in the Health & Safety File.

Scaffolding and Access Equipment

The Work at Height Regulations 2005

All work locations from which a person could fall shall be risk assessed in accordance with the above regulations and suitable and sufficient working platform, guard rails, etc. shall be provided to ensure and maintain a safe working environment.  All Access Equipment supplied and used for the construction works must comply with current Health & Safety Regulations, Guidance Notes (HSE INDG401) and relevant British Standards.

Scaffolding

Where scaffolding is required to provide access to carry out the work, a safe working platform shall be designed, constructed and inspected in accordance with SG4:05 produced by the NASC (National Access & Scaffolding Confederation).  Unqualified operatives must not be allowed to construct, dismantle or alter scaffolding.

A safe means of access and egress (including emergency evacuation) must be provided to all working platforms.

The scaffolding shall be designed to enable the planned tasks to be carried out safely, they shall be protected to prevent so far as is reasonably practical, unauthorised access to either the scaffold and/or the buildings structure, during normal and outside normal working hours.
If scaffolding is to be used as a temporary materials store; design details and calculations shall be submitted for checking prior to erection.

Scaffold Towers

These must be constructed and operated in accordance with the manufacturer’s recommendations.

Roof Working 

All work shall be planned, risk assessed and carried out in accordance with HSG33

Roof Work:-

· Provide a safe means of access to and from the work area/s.

· Provide safety guard rails to the roof verges, openings, voids and lantern roof lights, with toe boards and intermediate guard rails.

· Provide additional guarding above all pedestrian walkways and all access / escape doors by the use of debris netting, solid guard balustrades, brick guards and/or scaffold fans. 

Ladders

Note: To minimise the risk of unauthorised use of access ladders, all access ladders located at ground level outside of the secured building, must be removed from site or locked in a secure compound/lockup when the site is closed. 
Ladders/Step Ladders shall not be used to carry out work unless a suitable risk assessment has been carried out and a suitable method statement devised.
Site operatives must be able to reach the work without over reaching.

Ladders must be in good condition: free of damage, of industrial specification, secured at the top and bottom to prevent slipping, working from a solid level surface.

Roof ladders and crawl boards must be of industrial quality, meet the requirements of HSG33, be correctly positioned to allow the works to be carried out safely.
Manual Handling and Mechanical Handling

The construction operations should be planned where possible to avoid the need for manual handling or repetitive movements, to reduce the risk of injury to personnel, heavy large or bulky items should where possible be planned for moving and locating mechanically.

All manual handling that cannot be avoided shall be carried out in accordance with the Manual Handling Operations Regulations 1992 (as amended 2002) and guidance issued by the HSE (L23).

Components weighing 20kg plus, must not be lifted by a single person.  Blockwork and other walling materials shall be ordered in sizes of less than 20kg.
Manual Handling

All works where it is intended to complete the works manually shall be risk assessed in accordance with the Manual Handling Operations Regulations 1992 (as amended 2002) and work specific method statements provided.  The regulations require employers and the self-employed to:-
· Avoid hazardous manual handling operations, so far as reasonably practicable.

· Risk assess any hazardous manual handling operations which cannot be avoided.

· Reduce risk of injury, so far as is reasonably practicable.

· Provide information on the load to be handled.

Mechanical Handling and Lifting

All lifting operations shall be panned and carried out in accordance with the Lifting Operations and Lifting Equipment Regulations 1998 (LOLER).  Lifting operations shall be supervised and controlled by a competent person.
Mechanical plant shall comply with the requirements of the Provision and Use of Work Equipment Regulations 1998 (PUWER) and be operated by persons trained and certified in the safe use and operation of that plant or equipment, who understands its hazards and limitations in use.  All plant operators shall hold a relevant Certificate of Training.

Mobile Hand Held Telephones 

Under no circumstances should a hand-held mobile phone be operated by anyone whilst driving or operating a vehicle or contractors’ plant on the site.

The use of 2 way radio telephones (between banksman and machine operator) for the control of plant or equipment is allowed subject to suitable training and risk assessment of the works to be completed.  They shall not be used whilst walking across or working on the site, accessing scaffold, driving or operating vehicles, site plant, tools or machinery.
ID Badges
All operatives are to wear photographic ID badges and logo’d workwear.

Signing In
The Working Foreman will fill in the Site Attendance Register.

Ground Conditions
Ground Investigations have been carried out and the site is classed as inert.  A copy of the Ground Investigation will be kept on site.

No contamination or problems are expected.

If suspected contaminated land is encountered, work must cease and the problem reported to the Contract Architect.
Speed Restrictions
Site vehicles accessing and egessing the site should not exceed a 10mph speed limit.

Parking

Parking will be limited to adjacent roads.
Sign Posting
Clear signage will be provided.
Electrical Test Certificates

All Electrical Test Certificates will be handed over on completion day.

Restrictions on Working Times (as per planning approval application 2020/1251)
The working hours, when using plant machinery or equipment or for deliveries will be

· 8.00am to 6.00pm Monday to Friday 
· 9.00am to 2pm Saturdays 
· No works on Sundays or Bank Holidays

Personnel on Site

Only experienced personnel will be used on site.  All sub-contractors will be recognised companies qualified to carry out the work. 
Security
The Site Manager will be responsible for ensuring that the building and the site are left secure at the end of every working day.
A daily register will be kept for all operatives and visitors to the site.
Asbestos

Traces of asbestos cement deposits were found when doing trial holes. A RAM will be provided to cover this when carrying out any form of excavation.   If any suspected asbestos is encountered, work must cease and it must be checked by a competent person.

All O&P operatives are asbestos trained and attend a refresher course annually.
A copy of the Asbestos Register will be kept in the Site Cabin.
Safety Monitoring Arrangements
The following registers and checklists will be kept up to date on site to monitor safety; -

1. Weekly Site Safety Check List.

2. Health and Safety Induction Register.

3. Site Induction Sheets.
4. Breaches of Company Rules Register.

5. Scaffold Reports and Checklists.

6. Incident Investigation reports.

7. Accident Reports.

8. Method Statements Register.

9. Register of Sub-Contractor’s Method Statements and Risk Assessments.
10. Plant Checklists (i.e. Forklifts and Dumpers etc.)
11. Abrasive Wheels Register.
Reports of Accidents

The aim of this Safety Plan is to achieve zero accidents.

Any accidents are to be reported to the Contracts Manager so that they can be recorded in the appropriate manner and reported as necessary to the appropriate body.  RIDDOR regulations will be followed.
Reporting and investigating of accidents and incidents shall be copied in to Principal Designer and Client.
First Aid

A fully stocked First Aid box including eyewash will be kept in the site office.  

There will be a first aider on site at all times.
TRANSPORTING MATERIALS FROM COMPOUND TO SITE

A banksman will be present to supervise the Telehandler driver whenever materials are transported from the compound on the other side of Laithes Lane.

Busy times will be avoided.

Clear signage will be erected to give early warning to car drivers regarding construction site operations.
Communication and Liaison with Neighbouring Parties

Users of adjacent buildings will be notified of the works.

Risk of Access by Unauthorised Personnel

Contractors and sub-contractors’ staff will wear identity badges or clothing displaying company name.

Machinery, Tools and Fixed Plant

All mobile plant to be used in accordance with the Provision and Use of Work Equipment Regulations 1998 and to be properly maintained with a copy of a valid thorough examination certificate of which are listed in the site health and safety file. 

Electrical equipment is checked, maintained and PAT tested yearly.

Plant and equipment shall be immobilized when not in use or when site is closed.

Removal of Rubbish

Skips to be positioned within the site compound. 

Skips to be enclosed unless exceeding 5m distance from the building.
All rubbish will be taken by a licensed carrier to a registered tip and all waste transfer notes will be recorded and maintained. Hazardous Waste Consignment Notes shall be sent with any hazardous material taken from site.
Barriers and Warning Signs 
Barriers and warning signs will be provided as necessary to ensure Safety where pedestrian routes pass near to contractor’s routes and point of entry.

Noise and Dust

Noise on site will be kept to a minimum by muffling machines and equipment wherever possible.  Where this is not possible, all operatives will be provided with ear plugs of ear defenders.
DUST SUPPRESSION 
Dust suppression equipment will be used for all dusty operations.

Dust Suppression Bottles will be used with Stihl cutting saw. 

Extract Units for Small Plant will be provided for use with such items as circular saws etc.  

Permits to Work
Permits to Work are not required by the client.
Permits to work must be obtained from the Site Manager for the following:

1. Hot Work

2. Work on live mains services
Deliveries and Unloading
There are no restriction for deliveries.
All deliveries will be made into the compound via the entrances shown on the site plan.
Deliveries should be arranged in smaller delivery lorries and articulated vehicles will not be used.
All delivery lorries will be supervised by a banksman.

Parking

All parking will be on site.
Hot Work

No “hot work” is to be carried out without a Hot Work permit.  Permits to be obtained from the Site Manager.

Hot Work is the name for all work involving and using exposed heat source.
To comply with the Council’s Insurers current rules, when the above types of construction works are carried out on/within council premises, they shall be covered by a current work specific, Hot Work Permit.  See Appendix 2.

The permit shall be completed and issued by the Client or his representative.  (This duty may be delegated by the Client to The Principal Contractor on certain sites).  The permit shall be issued before the Hot Work commences and on each and every occasion that Hot Work takes place.   

The responsible operative shall inspect the works 30 minutes and 60 minutes after the Hot Work has been completed, to check that the area is fire safe, then sign, date and return the declaration on the permit.

The fully completed permits shall be returned to the Project Manager or his Representative before the contractor leaves site on that day.
No hot work is to be carried out in the last two hours of a shift the Site Manager must check all areas before leaving the site.
Existing Services
The locations of the existing statutory services serving the site are shown, where known, on the contract drawings.  We will make full investigations, prior to setting up site compounds and before starting any site works, to determine and confirm the exact location of any services which may affect, or be affected by the proposed construction works. 

CAT scans will be carried out to accurately to locate these services prior to commencing excavations.
Site Fire Safety Plan

Emergency Services Access Route

The emergency services access route will be kept clear at all times.

Fire Assembly Point
The fire assembly point will be in the site compound on Laithes Lane.
The Site Manager will do a head count for the construction site.
Fire Extinguishers
A fire extinguisher will be located in the site cabin and in each of the bungalows once the shell is complete.
PASSIVE FIRE PROTECTION 

Passive Fire Protection (PFP) is an important component of a building’s fire safety strategy.  The inspection of PFP forms part of a fire risk assessment required under the Regulatory Reform (Fire Safety) Order 2005.  PFP is designed to prevent fire spread within a building or separate areas of high risk.  Overall, its aim is to ensure that any Fire event is contained within its compartment of origin for a predetermined period of time.  It is therefore essential to ensure PFP is properly designed, installed and maintained in a building. 
A RAM will be provided to ensure this aspect is covered.
Office

A cabin will be provided in the position shown on the site layout plan.
Signposts will be posted to enable visitors to find the office.

The F10, Health and Safety Poster, insurances etc. will be posted on a notice board in the site office area.
All PPE and the First Aid box will be kept in this room.
SMOKING AREA 

A designated smoking area will be provided adjacent the site compound.

Welfare Facilities

A site cabin will be provided as shown on the site layout drawing.  Hot & cold running water and washing facilities will be provided within the building.
The facilities provided shall as a minimum comply with the requirements detailed in the HSE Information Sheet ‘Provisional of Welfare Facilities at Fixed Construction Site – Construction Information Sheet No. 59 (2011)
Sanitary Conveniences

A chemical WC unit will be provided with Hot & Cold Water.
These facilities will be maintained in a clean and hygienic manner.
Hot water is available in here.
Bottled drinking water will be provided when necessary.

Selection of Subcontractors
We have an approved list of subcontractors who are vetted as part of our Quality Assurance System to ISO9001.

All new subcontractors have to complete pre-qualification questionnaires.

Exchange of Health & Safety Information
All subcontractors will be provided with a copy of the Pre-Construction Safety Plan and Construction Phase Safety Plan with their order for the works.

The order will request copies of all appropriate RAMS two weeks prior to the relevant work commencing.

All subcontractors will be Health and Safety inducted on arrival and fill in an Induction Certificate.

Health and Safety co-ordination meetings will be held regularly throughout the contract period and Health and Safety notices will be posted on the Site Notice Board.

Exposure to UV Radiation from the Sun
Employees will be encouraged to keep covered up and will be instructed to apply sun block creams.  They will also be provided with information in the form of tool box talks should the sun make an appearance
Young Persons and Expectant Mothers
There will be no persons under the age of 16 allowed on the site unless by special arrangement. There will be no expectant mothers employed on the site.
Material Storage and Vehicle Parking

All materials used in construction will be stored in a steel lock up container within the compound and must be stacked and stored in a safe manner.

Consultation with Workforce on Health and Safety Issues

Following their briefing on the Health and Safety Plan the workforce will be encouraged to give their views on health and safety arrangements and any suggestions given will be considered by the Site Manager.

Operatives will be made aware that they should contact the Site Manager at any time if they are unsure of or unsatisfied with health and safety arrangements.

The above will be reminded to operatives and subcontractors during any subsequent tool box talks.

On Site Training

On site training will be provided in the form of tool box talks.

These talks will be given by the site manager on specific tasks or hazards.

Tasks requiring method statements will automatically be subject to a tool box talk as operatives are briefed on the method statement.
Talks on this project will include: -

a) Site cleanliness
b) Manual handling
c) Respect to neighbours regarding parking, noise and dust

7. OVERLAP WITH CLIENTS UNDERTAKING

The site will be vacant throughout the contract period.
8. SITE RULES
a) All power tools will be 110v or battery powered.  Direct connection to mains will not be allowed.

b) The site to be kept tidy at all times.

c) No smoking or E cigarettes will be allowed at any time within the curtilage of the premises.

d) Hard hats will be worn when overhead work is carried out.  Safety boots to be worn at all times.

e) The site to be left secure at the end of each day.

f) Highways, footpaths and all access areas to be kept clear of mud and debris at all times.

g) Dust masks must be worn when undertaking any dusty operation.
h) No burning of materials or rubbish will be allowed on site.  All rubbish must be placed in skips or removed directly by lorry.

i) Dust must not be allowed to escape from the working area.

j) No radios will be permitted at any times.

k) Existing roadway to be kept clean at all times.
l) All employees must adhere to the company Drug and Alcohol policy a copy of which is posted on the Site Notice Board.
9. CONTINUING LIAISON

Arrangements for Monitoring

The Contracts Manager will monitor and ensure adherence to the Health and Safety Plan.

Monthly site meetings will be arranged on site with all parties present.
Any changes in design which affect Health and Safety will be covered by an addendum to the Safety Plan and will be sent to the Principal Designer and all sub-contractors.
Design Alterations
All alterations to the design should be notified to the Principal Designer.  Designers should reassess risks and hazards when amending design and inform the Principal Designer and Contractor accordingly of any information that may subsequently affect maintenance, cleaning and ultimate demolition.
Health and Safety File

The Principal Contractor, Contractors or Designers in possession of information shall forward the same to the Principal Designer for inclusion within the Health and Safety file.  
Review of Procedures

A review will be undertaken on all site procedures for use on this and future projects.

FIRE PROCEDURE
CONSTRUCTION OF SEVEN BUNGALOWS AT  

LAITHES LANE, ATHERSLEY, BARNSLEY, S71 3AN

PROCEDURES IN CASE OF FIRE

FIRE ON CONSTRUCTION SITE
All O & P Construction Services Ltd staff will have been instructed on fire evacuation procedures, which will involve verbally informing all members of the constructions staff of the fire and instructing them to evacuate to the Fire Assembly Point.
The Site Manager will be responsible for carrying out a head count to ensure everyone has been evacuated.

FIRE ASSEMBLY POINT

THE FIRE ASSEMBLY POINT WILL BE IN THE COMPOUND ON LAITHES LANE.
OUR SITE MANAGER WILL DO A HEAD COUNT FOR THE CONSTRUCTION SITE.

CONSTRUCTION OF SEVEN BUNGALOWS AT  

LAITHES LANE, ATHERSLEY, BARNSLEY, S71 3AN
INDUCTION SHEETS
It is essential that you READ and UNDERSTAND the attached Health and Safety information

SAFETY INDUCTION 
CONSTRUCTION OF SEVEN BUNGALOWS AT  

LAITHES LANE, ATHERSLEY, BARNSLEY, S71 3AN

The contractor must ensure that all new contractors and visitors to site undertake safety induction.  The induction must include information regarding the following safety considerations and include any other Client specific requirements.

	Item for safety consideration
	Item covered
	Item for safety consideration
	Item covered

	Introduction to the Work Supervisor
	
	Site rules
	

	Overview of the project
	
	Emergency/escape procedures
	

	Site boundaries and no go areas
	
	Fire safety procedures
	

	Site access and egress
	
	Fire alarm system & Fire muster point
	

	Site access for deliveries
	
	CSCS/ CPCS/ Licences 
	

	Use of site vehicles (plant access roads)
	
	Alcohol and drug exclusion policy
	

	Materials storage areas
	
	Good housekeeping and tidy site policy
	

	Storage of flammable substances
	
	Procedures for any work at height
	

	First aid station
	
	Use of scaffold, working towers etc.
	

	Welfare facilities on site
	
	Use of small tools on site
	

	Site electrical supply
	
	Specific high risk work on site
	

	Smoking area & No E-Cigarettes Policy
	
	Environmental requirements for site 
	

	Request information of any Medical conditions
	
	Reduce, reuse, recycle
	

	Considerate Constructor Scheme 

(where applicable)
	
	RESPECT!! Treat people, equipment and the environment how you expect to be treated.
	

	Health and Safety Notice Board
	
	Face Fit Testing – FFPS Masks
	

	

	Name
	CSCS/CPCS
	Contractor
	Signature
	Date
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