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METHOD STATEMENT

PROCESS
Measures to control the emission of dust and dirt during the construction
METHOD
1. All operatives are to use dust extraction and respiratory equipment whilst undergoing work.

2. [bookmark: _GoBack]Tradesman will provide themselves with all 110v equipment connected to the extraction units if needed.
MEANS OF SAFE ACCESS
Access to the working area will be via the front/rear doors of the premises.

PERSONAL AND RESPIRATORY PROTECTIVE EQUIPMENT
Tradesmen will be provided with necessary PPE and RPE by Whitshaw Builders Ltd. including ear
defenders, protective gloves, gauntlets, eye protection, hard hat, safety boots, high
visibility vest, knee pads and respirator/dust mask. Tradesmen will wear high visibility vest and safety boots at all times on site. Specific PPE requirements are detailed in the method statement above.

Tradesmen will assess the need for using additional items for each part of the operation and have
been trained to do so. Any mandatory site safety requirements will be complied with.
ELECTRICAL EQUIPMENT
110-volt equipment only will be used. This is to be visually inspected for damage by tradesmen at
the commencement of each working day and to be within test date.
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