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PROJECT HSEQT
ACTIVITY RISK ASSESSMENT

	Project Name & No.:
	B&B Barnsley
	Risk Assessment No.:
	RA.MS- BAR - 001

	Risk Assessment Title:
	New road layout
	Revision No.:
	



	Specific Location of Works:
	Huddersfield Road
	Anticipated Start Date of Works:
	TBC

	Scope & Description of the Works:
	New road layout

	Associated Documents:
	MS-BAR-001 

	Risk Assessment Completed by:
	Name: Gary Smith
	Signed: Gary Smith
	Date: 06/12/16

	Risk Assessment Reviewed by:
	Name: George Mowbray
	Signed: George Mowbray
	Date: : 06/12/16 


	Likelihood Rating Key:
	Severity Rating Key:
	
	
	Severity Rating

	
	
	
	
	5
	4
	3
	2
	1

	5
	Frequent [1 or more per week]
	5
	Multiple or Single Fatality or Collapse of Structure
	Likelihood Rating
	5
	25
	20
	15
	10
	5

	4
	Probable [1 per month]
	4
	Major Injury or Major Damage to Property
	
	4
	20
	16
	12
	8
	4

	3
	Occasional [1 per year]
	3
	Reportable Lost Time Injury or Significant Damage to Property
	
	3
	15
	12
	9
	6
	3

	2
	Remote [1 in 10 years]
	2
	Other Lost Time Injury or Damage to Property
	
	2
	10
	8
	6
	4
	2

	1
	Improbable [1 in 100 years]
	1
	Minor Injury
	
	1
	5
	4
	3
	2
	1

	Residual Risk Rating Matrix Key:

	12 – 25:
	Unacceptable level of risk.  Risk level MUST be reduced.  Operations WILL NOT proceed until the level of risk is reduced to an acceptable level.  Requirement for the works need to be reviewed and alternative methodologies investigated where risk cannot be reduced to an acceptable level.

	5 – 11:
	Risks acceptable where principles of prevention have been applied and control measures implemented to reduce risk so far as is reasonably practicable.  Activity, operation or works creating the hazard and risk must be managed and supervised to ensure continued effectiveness and compliance with the control measures.

	1 – 4:
	Acceptable level of risk.  Risk associated with the hazard is considered to be of an acceptable level.  Continual reviews to confirm hazards and risks remain adequately controlled.


	1:  Hazard Description
	2:  Person[s] at Risk
	3:  Potential Consequence[s]
	4 – 6:
Initial Risk Rating
	7:  Control Measure[s]
	8:  Person[s] Responsible for Implementation & Monitoring
	9 – 11:  Residual Risk Rating

	
	
	
	L
	S
	IRR
	
	
	L
	S
	RRR

	Contact with Contaminants 


	Site Operatives
	Occupational Health problems resulting in Major injury
	3
	4
	12
	COSHH assessments available and briefed to all operatives

Adequate toilet & wash (to include hot and cold or running water) facilities, Areas provided to eat food / store clothes

Regular maintenance on facilities to ensure kept clean


	Project Manager

Foreman

Site operatives
	1
	4
	4

	Fire / Explosion due to exposure of flammables to source of ignition 


	Site Operatives, other persons on site  
	Major injuries, fatalities
	4
	5
	20
	No smoking, Switch off engines, lights and mobile phones, Use only approved containers,

Replace hoses after use

Drip trays, 

Authority required to receive fuel
	Project Manager

Foreman

Site operatives
	1
	5
	5

	Slips/Trips


	Site Operatives, other persons on site  
	Major & Minor injuries
	3
	3
	9
	Use only approved containers,

Replace hoses after use in storage facility

Drip trays, plant nappy’s

Authority required to receive fuel, 
	Project Manager

Foreman

Site operatives
	2
	3
	6

	Fence collapse or blown over
	Site Operatives
	Major injury
	3
	4
	12
	All fencing to be double clipped. Stays to be adequately positions, regular inspection by the site management team to ensure stability, especially after adverse weather conditions.

Ensure all signs are adequately fixed in position to prevent accidental or unauthorised removal
	Project Manager

Foreman

Site operatives
	1
	4
	4

	Plant Movement
	Site Operatives
	Major injury
	4
	4
	16
	Competent & trained operators, banksmen/vehicle marshals in place.  Segregation of plant & pedestrians at all times.  


	Project Manager

Foreman Appointed Person

Vehicle Marshal
	1
	4
	4

	Failure of Lifting accessories
	Lifting operations team
	Fatality

Major & Minor Injury
	3
	5
	15
	Certified lifting accessories, recorded on site lifting register

Weekly inspections by site management team

Recertification every 6 months

Stored correctly at all time when not in use

Do not store in excavator tool bins at any time

Remove from use should damage occur, lock in a designated disposal bin.


	Project Manager

Foreman Appointed Person

Crane Supervisor

Banksman
	1
	5
	5

	Manual Handling
	Site Operatives
	Back injury
	4
	3
	12
	Manual handling assessment carried out and briefed to all operatives.
	Project Manager

Foreman
	2
	3
	6

	Identify / contact with underground utility services e.g gas /elec / bt etc

	Site Operatives
	Short circuit , explosion resulting in Major injury, fatality
	4
	5
	20
	DABS, RAMS method statement briefing
All opp’s trained & competent
Permit to break ground issued
Full CAT & Genie Scan of work area
Utilities identified and marked
	Site Manager / Supervisor / Foreman

HSEQT Advisor
	1
	5
	5

	Dumper overturning


	Site Operatives
	Trapping body / Major Injury, Fatality
	3
	5
	15
	Only to be driven by trained and competent operators, site speed limits, Beacon to be attached and working, Daily pre-use inspections Avoid steep gradients

Do not discharge load on a gradient,

Never drive with excess loads
	Site Manager, Safety Supervisor/Foreman

HSEQT Advisor
	1
	5
	5

	Silica Dusts generated by cutting operations


	Site Operatives


	Respiratory illness, major illness
	2
	4
	8
	Dampen dusts

Ensure equipment suitable for work and maintained

PPE including goggles, dust mask etc

Area of works barriered off correctly and signed
	Project / Site Manager

HSEQT Advisor
	1
	4
	4

	Lifting kerbs


	Site operatives
	Back or other manual handling type of injury ( Muscular-skeletal injuries)
	4
	3
	12
	No manual handling, all lifts to be with kerb layer

All staff trained

Equipment maintained


	Project / Site Manager

HSEQT Advisor
	1
	3
	3

	Lifting / adjusting kerbs
	Site operatives
	Minor Cuts & Abrasions
	4
	2
	8
	No manual handling, all lifts to be with kerb layer

All staff trained, PPE


	Project / Site Manager

HSEQT Advisor
	2
	2
	4

	Failure of mechanical means of lifting resulting in impact with operative
	Site operatives
	Minor injuries
	3
	2
	6
	Equipment maintained

All staff trained, PPE


	Project / Site Manager

HSEQT Advisor
	2
	2
	4

	Working near drains / waterways or other higher risk locations


	Site Operatives
	Contact with water contaminated with infected rats urine 
	3
	5
	15
	Induction 

Information & training.

Adequate PPE.

Cover all cuts and abrasions.

Dispose of biological waste properly


	Site Manager / Supervisor

HSEQT Advisor 
	1
	5
	5

	    Bursting of wheel  

   disc / Flying particles


	 Site Operatives
	 Eye injuries

 Lacerations Burns
	3
	4
	12
	Wheel mounting & use by trained / competent operatives, Machine Guards,

Pre-use inspections

Appropriate PPE
	Site Manager,  Safety Supervisor / Foreman

HSEQT Advisor


	1
	4
	4

	    Contact with the 

    wheel or disc


	Machine Operator or other Site Operatives
	 Lacerations
	2
	3
	6
	Use by trained / competent operatives

Pre-use inspections

Use of suitable Guards
	Site Manager,  Safety Supervisor Foreman

HSEQT Advisor


	1
	3
	3

	   Entanglement of 

   loose clothing


	Machine Operator
	Fractured Limbs / Fingers 
	2
	3
	6
	Use of suitable Guards.

Wheels and discs marked with correct speed & fitted correctly, PPE 


	Site Manager,  Safety Supervisor Foreman

HSEQT Advisor


	1
	3
	3

	Excavations  -  Collapse of trench / falling materials


	Site Operatives 
	Collapse of trench / falling materials resulting in fatality, Major Injuries 
	5
	5
	25
	DABS, RAMS

Trained & competent staff

Permit to Dig

Permit to Enter

Adequate support systems, HSEQT  Audits & Inspections 

Store materials away from excavation
	Site Manager / Supervisor / Foreman

HSEQT Advisor 
	1
	5
	5

	General site activities

Persons falling from height into excavation


	Site Operatives
	Persons falling from height into excavation resulting in Major Injuries
	5
	4
	20
	DABS, RAMS

Excavations to be  protected by barriers / fencing, Lighting 
	Site Manager / Supervisor / Foreman

HSEQT Advisor
	1
	4
	4

	Working in a noisy environment


	Site Operatives
	Tinnitus, reduction in hearing ability, deafness Major injury
	4
	4
	16
	DABS, RAMS,

Trained & Competent personnel, If noise levels exceed 80 dB(A) Notify employees hearing protection advised

If over 85 Db(A) Hearing protection mandatory,

Post Warning Signage, Silenced plant, Screen off area.

Health surveillance 

Area barriered off, Well 

PPE  
	Site Manager / Supervisor 

HSEQT Advisor 
	1
	4
	4
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