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[bookmark: _Toc202365948]1.0 Introduction

1.1 This Construction Management Plan sets out the proposed approach to traffic management for the construction of the proposed River Dearne footbridges and includes details of:

· Indicative working arrangements including vegetation clearance, earthworks, construction
· The parking of the vehicles of site operatives and visitors;
· Loading and unloading of plant and materials;
· Management of construction traffic and access routes – including traffic transporting fill material to the site;
· Storage of plant and materials used in constructing the development;
· Measures to prevent mud/debris from being brought onto the adopted highway;
· The hours during which construction activities shall take place (which shall be between 08:00 and 18:00 on Mondays to Fridays and 08:00 and 13:00 on Saturdays unless otherwise agreed);
· A scheme for the control of construction site noise;
· A project description and likely sources of dust emissions;
· Roles and responsibilities for ensuring minimisation of dust emissions;
· Measures to be adopted to minimise dust emissions;
· Incident logging and reporting procedures.

[bookmark: _Toc202365949]Summary of Project

1.2 The Strategic Transport Service has received over £40m from the City Region Sustainable Transport Settlement fund (CRSTS) to deliver a programme of work, including active travel routes around the Barnsley Borough. This includes the development of the construction of the River Dearne Long Route and the replacement of two footbridges in the Dearne Valley Country Park which will provide improved access for pedestrians, wheelchair users and cyclists.

1.3 Improving active travel opportunities, into the town centre, reducing congestion and traffic are central themes in plans to tackle modal shift and the climate emergency in the borough. This route and the replaced footbridges form an integral part of a comprehensive network of proposed new walking and cycling routes across the borough.







[bookmark: _Toc202365950]Site Description

1.4 The site is situated approximately 2km from Barnsley town centre within the Dearne Valley Country Park (Site LNR3) and includes land on both banks of the River Dearne. The site can be accessed by vehicle via a car park off the A628 Pontefract Road and Lord Street.

1.5 The Country Park includes a network of footpaths and through the City Region Sustainable Transport Settlement (CRSTS) the River Dearne Long Route has been  widened and resurfaced.

1.6 There are currently three footbridges within the Park that cross the River Dearne, 2 of which are narrow and not LTN1/20 compliant and do not provide sufficient width to allow cyclists or other users to pass.

1.7 BWB Consulting were appointed to inspect the existing bridges and to provide the Council with information on their structural stability for either improvement or whether a new footbridge should be provided. Their report concluded that, given the damage to the existing abutments and the issue of river scour, replacing the bridges with new bridges and abutments outside the influence of the existing bridges.

[bookmark: _Toc202365951]Development Description

1.8	The development will consist of replacement of 2 footbridges with new, all users, accessible bridges crossing the River Dearne, roughly in their current locations. All access ramps will connect into the existing footpaths that cross the Country Park.

1.9	The ambition of the scheme is to create a safer and more accessible river crossing that enables better movement for a variety of users. The proposed scheme joins the existing River Dearne Long Route (PRoW 217) which runs through the Country Park and provides links to residential areas north of the park.

1.10	BWB were tasked with looking at the various options for either replacement bridges on the existing abutments or to design a totally new bridge in a new location. Given the need to reduce the environmental impact in the Dearne valley park it was agreed that replacement bridges that were LTN1/20 compliant was preferred.

1.11	The replacement bridges will be constructed from steel, which is a standard material for a river bridge and will be in keeping with the character and appearance of the surrounding area.

[bookmark: _Toc202365952]Key Contacts

1.12 The following people will act as the key contact for the development works which are being carried out and they will be the main point of contact for any complaints which are received during the programme of works:
•	Client –Barnsley Metropolitan Borough Council
•	Principal Contractor – to be confirmed
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2.1 The Principal Contractor shall have procedures in place to deal with incidents involving environmental issues relating to site works. 

2.2 All incidents shall be recorded and reported to the Project Manager as soon as practicable and at least within 24 hours of the incident occurring, and if appropriate, reported to the EA. A follow-up report shall also be produced providing details of all relevant information.  

2.3	Environmental incidents shall be reported to the EA and the Statutory Authorities as required. In line with the following requirement:
‘When reporting an incident, the following information must be included (when reporting out of hours, only brief personal/incident details should be left on the answer phone service and the remainder captured during normal working hours)’:

· Name, job title and contact telephone number of the manager/person reporting;
· Operational Depot/Business Department/Directorate;
· The name of the operative or member of public involved in the accident or incident;
· Employee status: direct labour or contact labour;
· Operative job title and the type of work activity being undertaken at the time of the incident;
· The relevant Manager/First Line Report;
· The date and time of when the incident occurred;
· A brief factual description of what happened (do not speculate or make assumptions). For security related incidents, this should include any items stolen (with an estimate of the cost), crime reference numbers and police details; and,
· Details of actions already taken to safeguard individuals and the public
· A follow-up report should also be produced providing details of all relevant information. 

2.4 The principal contractor shall report the discovery of deleterious materials, for example, asbestos, fuel oils, etc. to BMBC after testing by an appropriate accredited laboratory. All hazardous discoveries shall be entered into the method statements for the relevant project.  Attention must also be drawn to any specific company or Statutory Authority requirements, which may detail actions to be taken.
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3.1	This section of the CEMP has been designed to specifically deal with the following:	 
· The parking of the vehicles of site operatives and visitors;
· Loading and unloading of plant and materials;
· Storage of plant and materials used in constructing the route.
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3.2	Access to the site is through the existing access from the A628 Pontefract Road and the Dearne Valley Country Park Car Park No.1 . 

[bookmark: _Toc202365956]Vehicle Parking Details

3.3	The clear establishment of an appropriate construction compound and parking area is required to prevent and minimise the disruption to the local residents and users of the Dearne Valley Country Park as far as possible.

3.4	It is proposed that a construction compound including a vehicle parking area, will be situated on land adjacent to Car Park No.1. The standard layout of the construction compound is shown in Appendix A.	Comment by Edwards , Jake (PROJECT OFFICER/ PROJECT MANAGER): Neil to complete, awaiting BWB to be commissioned for detailed design

3.5	It is anticipated that this area can be utilised throughout the entire replacement of the bridges. However, if at any stage during the works a new compound is required, the Principal Contractor will submit plans and agree in writing with BMBC a revised area.

3.6	Vehicle parking associated with the construction works will not be prohibited on other areas within proximity to the scheme unless otherwise agreed with the BMBC. No vehicle parking will be permitted at any stage on public highways within the vicinity of the scheme.

3.7	The vehicle parking area will be positioned within the contractors compound to minimise the disturbance of the surrounding area. The parking area will be positioned immediately next to the access road to reduce the amount of vehicular movement on site and therefore reduce the likelihood of vehicles taking mud/debris onto the existing highway network when they leave the site.

3.8	To prevent spills from oil and fuel from any vehicles occurring within the compound and subsequently entering the groundwater/ surface water drains, the following measures will be adopted;
•	Plant nappies will be utilised to collect leaks from diesel pumps or from standing plant;
•	Oil/fuel interceptors will be fitted to all temporary discharge points from the compounds and from any temporary oil storage or refuelling areas; and,
•	Within the construction compound there will be the provision of spill containment equipment such as absorbent material.

[bookmark: _Toc202365957]Construction Workers Compound

3.9	The construction workers compound will provide an area for storage of plant and materials and welfare facilities separate from construction activities. 

3.10	Appropriate security fencing or hoardings will be provided around the perimeter of the compound. Fence type and construction will depend on factors such as the level of security required, the likelihood of intruders, and the degree of visual impact.

[bookmark: _Toc202365958]Deliveries

3.11	A designated area will be situated within the compound for the specific loading and unloading of materials and plant. This will be the most appropriate location as the compound is in close proximity to the access road and is also the location where materials and plant will be stored.

•	Deliveries will report to the site office and all delivery drivers will sign in and out on completion of delivery.
•	Banksmen will be present during reversing operations, where operator's view is obscured. Flashing beacons will be fitted to all on site vehicles and plant.
•	Plant is to be fitted with traverse alarms to ensure safe manoeuvring.

3.12	Where deliveries are required for bringing in materials which are required for the foundations, subgrade, sub-base or surface layers, these materials will be delivered on a ‘as required’ basis and will be taken directly to the location they are needed rather than being stored and subject to being moved again
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4.1	This section of the CMP has been designed to specifically deal with the following: 

· 	Management of construction traffic and access routes – including traffic transporting fill material to the site.
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4.2	Access to the site is through the existing access from the A628 Pontefract Road and the Dearne Valley Country Park Car Park No.1 .

4.3	Should it become apparent at any point during the construction programme that an alternative access is required, details of this change would be submitted and agreed in writing with BMBC prior to making these changes.

4.4	The clear establishment of an appropriate traffic access to the Site is required to prevent the likelihood of accidents occurring and to minimise the disruption to the local residents and road users as far as possible. 

4.5	The specific measures below will be implemented to reduce the impact of construction traffic both on and in the wider areas surrounding the Site:

•	The principal contractor must agree the principles and routes for material haulage to and from The Site with the Local Highways Authority as appropriate; 
•	The contractor will operate a traffic management system across the Site, which is relayed to all personnel during induction. The traffic management plan and routes will always be visible at the site entrance and will indicate the location of the site office;
•	A noticeboard will be visible at the site entrance to inform of hazards and any changes to the traffic management plan;
•	The provision of temporary signalling should be considered where vehicle access to the Site is likely to cause congestion or the potential for access;
•	The movement of construction vehicles should be limited to non-peak hours where possible to limit any disruption to the local highway network;
•	All construction traffic entering and leaving the Site shall be closely controlled and HGVs making deliveries to the Site or removing construction material etc, shall avoid prohibited routes;
•	Vehicles should be loaded and unloaded clear of the public highway;
•		Deliveries will be scheduled for outside of peak times to avoid any potential disruption to traffic; and,
•	The Labour force shall be encouraged to car-share and to use sustainable modes of transport. 
· 	Access routes through the Site will be maintained clear to enable unrestricted access to foot / vehicular traffic, including the Emergency Services in the event of an emergency.
· 	Emergency escape routes will be designated prior to commencement of work.
· 	All persons visiting the Site shall be logged in and out.
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4.6	Given the number of HGV’s which are likely to be required to facilitate the works, there is a necessity for the construction traffic coming to the site to use the main A628 Pontefract Road and not take short cuts through adjacent neighbourhoods.

4.7	As a result the principal contractor should ensure that the deliveries are made to site using the most appropriate routes which should by via the M1 where possible and then onto the A628.




5.0 [bookmark: _Toc202365962] Cleanliness of Public Highways

5.1 This section of the CMP has been designed to specifically deal with the following:

· Measures to prevent mud/debris from being brought onto the adopted highway;
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5.2 Roads in the surrounding area are currently subject to standard Council maintenance and will be periodically cleaned.

5.3 Recommendations for suppression of dust and dirt are also covered in Section 8 however, a summary of these measures are also provided below.

5.4 The construction works will involve the regular use of the local highways network by construction related vehicles. As such it is imperative that measures are put in place to minimise the deposition of mud and debris on the local road network generated by vehicular movements. These measures are outlined below:

· Wheel wash facilities should be provided near to the Site’s access and egress points to ensure that vehicles are appropriately cleaned prior to accessing public highways.  The type of wheel washing facilities should be appropriate to the types of vehicles being used on the Site and the amount of mud and debris likely to be on the vehicles. However, as a minimum the wheel washing facilities should comprise a manually operated high pressure jet wash.
· The specific locations and types of wheel washes to be used on the Site should be submitted and agreed with BMBC at least four weeks prior to commencement of the works on Site.
· Wheel wash areas should be contained and appropriately disposed of to prevent suspended solids or contaminated waters from entering any nearby water courses or drains. To dispose of this water, it will be necessary to obtain the consent of the EA to discharge into the foul sewers, or if the water contains contaminants such as oil or fuel it will need to disposed of as controlled waste.
· All vehicles leaving the Site should be subject to a visual inspection before accessing the public highways to ensure that the level of dust/mud/debris on the vehicles has been minimised insofar as is practical.

5.5 It will be the responsibility of the contractor to undertake a daily inspection of the adjoining roads.  All road surfaces affected shall be swept clean upon completion of the works.
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6.1.	This section of the CMP has been designed to specifically deal with the following: 

· The hours during which construction activities shall take place (which shall be between 08:00 and 18:00 on Mondays to Fridays and 08:00 and 13:00 on Saturdays unless otherwise agreed)
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6.2	The A628 Pontefract Road is likely to be busy throughout the day, but especially around the hours of 07:00 and 09:00 a.m. and 16:00 and 18:00 p.m. during the morning and evening rush hours.

6.3	It is proposed that the following times will constitute the normal working hours (excluding public holidays) as specified within Condition 4 on the construction site:-
•	Monday to Friday, 08:00a.m. to 18:00p.m.; and,
•	Saturday’s, 08:00a.m. to 13:00p.m unless otherwise agreed. 
· No work shall take place on Sundays or bank holidays.
6.4	These times will be displayed prominently on site notices on the boundary of the site, on display to all. Details of working hours will be included with correspondence with neighbours.
 
6.5	These hours will be followed unless otherwise agreed in writing by BMBC.  Outside the above periods the following working is permitted;

· pre-planned construction works to highway infrastructure or significant movement of materials or plant on the local highway network where first notified to BMBC and local residents;
· emergency works; 
6.6	Any emergency works carried out must be notified to BMBC within 72 hours of their commencement.
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7.1	This section of the CMP has been designed to specifically deal with the following: 

· A scheme for the control of construction site noise; 
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7.2	The Site is located within the Dearne Valley Country Park and is some distance from the nearest residential area.

[bookmark: _Toc202365968]Relevant Legislation and Policy

7.3	Any noise or vibration related work needs to adhere to the following environmental legislation:
•	Pollution Prevention and Control Act 1999; and,
•	The Control of Noise at Work Regulations 2005.

7.4	The construction works need to adhere to the following noise and vibration guidance;
•	BS5228-1:2009 ‘Code of practice for noise and vibration control on construction and open sites – Part 1: Noise’;
•	BS5228-1:2009 ‘Code of practice for noise and vibration control on construction and open sites – Part 2: Vibration’;
•	Environmental good practice on site, CIRIA C502, 2002; and,
•	PPG06 – Working at construction and demolition sites.

[bookmark: _Toc202365969]Construction Noise

7.5	 ‘Best Practicable Means’ and the guidance provided within BS:5228 are to be employed to minimise construction impacts, including, for example:
•	No deliveries should occur outside of the hours identified above unless agreed with BMBC;
•	Careful selection of working methods and programme;
•	Where applicable, selection of quietest working equipment available;
•	Where practicable, positioning equipment behind physical barriers, i.e. existing features, hoarding etc;
•	Ensuring that regularly maintained and appropriately silenced equipment is used;
•	Handling all materials in a manner which minimises noise, such as minimising drop heights;
•	Switching all audible warning systems to the minimum setting required by the Health and Safety Executive.  
•	Reverse warning alarms should be fitted with white noise (broadband) systems;  
•	Where processes could give rise to significant levels of noise for extended periods of time, noise levels should be monitored regularly by a suitably qualified person with the survey results kept on file; and, 
•	In terms of on-site employees, appropriate actions should be undertaken with regard to the Noise at Work Regulations including the requirement for the use of ear defenders and appropriate warning notices.  

7.6	Further to the above, operatives should be trained to employ appropriate techniques to keep site noise to a minimum and should be effectively supervised to ensure that best working practice in respect of noise reduction is followed.  All employees should be advised regularly of the following, as part of their training:

•	The proper use and maintenance of tools and equipment;
•	The positioning of machinery on site to reduce the emission of noise to the neighbourhood and to site personnel;
•	The avoidance of unnecessary noise when carrying out manual operations and when operating plant and equipment;
•	The protection of persons against noise; and, 
•	The operation of sound measuring equipment (selected personnel).

7.7	Measurements of construction noise must be undertaken in accordance with BS 5228:2009 – “Code of Practice for Noise and vibration control on construction and open sites” (Part 1 – Noise) at a noise sensitive receptor. 

[bookmark: _Toc202365970]Construction Vibration

7.8	Unless otherwise agreed by BMBC, all construction works must comply with the guideline vibration limits below.  Measurements must be undertaken at any occupied building within or outside of the Order limits within a distance of 25m from piling or any works likely to cause elevated levels of ground borne vibration to ensure compliance with the guideline limits.  Measurements must be undertaken in accordance with BS 5228:2009 – “Code of Practice for Noise and vibration control on construction and open sites (Part 2 – Vibration)” and BS7385:1993 – “Evaluation and measurement for vibration in buildings (Part 2 – Guide to damage levels from ground-borne vibration)”. 

[bookmark: _Toc202365971]Toolbox Talks

7.9	The Principal Contractor would be required to provide a tool box talk on methods to reduce the effects of noise and vibration to both construction workers and local sensitive receptors. 

[bookmark: _Toc202365972]Complaints
7.10	Prior to the commencement of construction works at the Site a ‘complaints hot-line’ should be set up to allow local residents and members of the public to voice any concerns which they may have regarding the noise levels from the construction. The details of this phone number should be displayed on appropriate signage at the Site entrance. 

7.11	In the event that complaints for noise nuisance are received by BMBC which considers those complaints justified, the contractor must unless otherwise agreed by BMBC, at its own expense, employ a consultant approved by the council to carry out an assessment of noise from the construction works.  The assessment will be carried out to an appropriate methodology agreed in writing by the Environmental Health Officer at BMBC and the results of the assessment submitted within 28 days of the assessment.  Those results must include a comparison of measured data with the requirements, all data which was collected for the purposes of the assessment and certificates of the measuring instrument’s calibration.
 




[bookmark: _Toc202365973]8.0	Control of Dust and Other Emissions 

8.1	This section of the CMP has been designed to specifically deal with the following: 

· 	A project description and likely sources of emissions; and,
· 	Roles and Responsibilities for ensuring minimisation of dust emissions;
· 	Measures to be adopted to minimise dust emissions
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8.2	The construction of the footbridge and the embankments will involve a significant amount of earthworks a to provide a level and stable abutments for the bridge, followed by the construction and lifting of the new bridge into place. During these activities there will be a significant amount of plant and HGV movement.

8.3	The main source of emissions during construction are likely to be dust and particulate matter generated during the earthworks (particularly during dry months) or from construction materials. The main potential effects of dust and particulate matter are:

•	Visual – dust plume, reduced visibility, coating and soiling of surfaces leading to annoyance, loss of amenity, the need to clean surfaces;
•	Physical and/or chemical contamination and corrosion of artefacts;
•	Coating of vegetation and soil contamination; and,
•	Health effects due to inhalation e.g. asthma or irritation of the eyes.

8.4	A number of other factors such as the amount of precipitation and other meteorological conditions will also greatly influence the amount of particulate matter generated.

8.5	Construction activities can give rise to short-term elevated dust/PM10 concentrations in neighbouring areas. This may arise from vehicle movements, soiling of the public highway, demolition or windblown stockpiles.

[bookmark: _Toc202365975]Relevant Legislation and Policy 

8.6	Any works likely to generate dust or emissions needs to adhere to the following environmental legislation:

•	Clean Air Act 1956; and,
•	Pollution Prevention and Control Act 1999.

8.7	The construction works need to adhere to the following air pollution guidance:

•	Guidance on the Assessment of Dust from Demolition and Construction, IAQM, 2014.
•	Environmental Good Practice on site, CIRIA C502, 2002; and,
•	PPG06 – Working at construction and demolition sites.
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8.8	In order to minimise the potential impact on air quality, the contractor shall adhere to the measures outlined below. If any deviation to these measures is required for any reason, the contractor will submit the amended requirements, along with the appropriate justification in writing to the BMBC formally agree these changes.

8.9	In order to prevent dust nuisance particularly during dry and windy weather, there should be adequate screening and damping down during all demolition works and other site preparations (including storage of construction materials).
•	All rubbish skips will be exchanged on a regular basis and sheeted when required;
•	Vehicles shall be sheeted to prevent loss of materials off site;
•	Storage locations should be aggregated where practical to avoid the creation of many stockpiles, adequately screened to prevent wind loss and damped down where practical when being handled;
•	Waste materials shall not be burnt on-site;
•	Wastes must be placed in suitable containers prior to appropriate disposal; 
•	Sweeping should be done regularly to prevent the build up of fine waste dust material; and,
•	Prolonged storage of materials on site prior to use and/or disposal is to be avoided.

8.10	Given the nature of the works, the construction of the development may involve the use of construction vehicles and HGV’s. Whilst there is only a single access point to the Site, it is imperative that measures are put in place to minimise the dust generated by vehicular movements. These measures are outlined below.

•	Prior to leaving site, each vehicle will be assessed for mud and dust. Wheel wash facilities will be provided at the Site access point to ensure that vehicles are appropriately cleaned prior to accessing public highways. The type of wheel washing facilities should be appropriate to the types of vehicles being used on the Site and the amount of debris likely to be on the vehicles. 
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8.11	  Mobile plant should be located away from sensitive receptors near to the Site.

8.12	Lorries and plant with diesel engines on or off site should be well maintained in order to reduce emissions of visible smoke.

8.13	Engines should not be left idling unnecessarily, and plant and vehicles must not be parked in a position that could give rise to nuisance from exhaust fumes.

8.14	 Site machinery and vehicles should use low-emission fuels where practicable.

8.15	Site vehicles and plant with low exhaust emissions (e.g. with particle traps) and emission controls such as catalysts or diesel particle filters should be used.

8.16	Contractors should take all precautions to prevent the emissions of fumes from stored fuel oils, for safety and potential nuisance reasons. 
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8.17	A toolbox talk will be delivered to contractors in respect to potential dust and other emissions effects.

[bookmark: _Toc202365979]Monitoring and Communications Recommendations

8.18	The following monitoring recommendations should be adhered to and records retained onsite to provide an auditable trail:

•	Records of dust and air quality complaints shall be kept, including likely causes and mitigation measures to reduce impacts if appropriate;
•	Daily on-site and off-site visual inspections shall be undertaken and recorded;
•	Notify local community of works hours and any specific works which are likely to generate higher levels of dust/emissions; and,
•	Notify local community of appropriate details to make complaints if necessary; Inspections should be increased during dry and windy weather and/or during periods of high activity (vehicular or earthworks) which is likely to increase sources of dust and emissions. 
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9.1	The following good practice measures are recommended in regards to storage of plant and materials and to enable pollution prevention

[bookmark: _Toc202365981]Storage of Fuel, Oil and Other Chemicals

9.2	The contractor will be required to develop detailed method statements for key aspects of work and handling of materials/liquids which have a potential for environmental impact. These should encompass proposals for the control of pollution, together with emergency response plans. The contractor will be required to observe and adhere to relevant legislation and guidelines. 

9.3	Plant and equipment will be stored in areas which are less susceptible to pollution and should be stored on a hardstanding base within the secure compound as agreed by between the contractor and BMBC.

9.4	Immobile plant, fuels, oils and chemicals will be stood on plant nappies or be secured/locked in appropriately bunded areas (at 110% of volume). Refuelling operations will be carried out within the designated construction compound remote from surface drainage systems. Leaking or empty drums will be removed from Site at once.

9.5	Specific measures for ensuring the prevention of polluting surface water are detailed in Section 10. 

[bookmark: _Toc202365982]Toolbox Talks

9.6	A toolbox talk will be delivered to contractors in respect to potential effects of pollution events.

[bookmark: _Toc202365983]Emergency Measures and Reporting of Incidents

9.7	The site staff will regularly inspect the site area for spillages. Spillage kits will be readily available and wet handling methods should be used to clean any spillages. 

9.8	Environmental incidents shall be reported to the Client’s Team and the relevant Statutory Authorities as required and anyway within 12 hours of the incident occurring. 

9.9	A follow-up report shall also be produced providing details of all relevant information. 

9.10	The contractor must have an accident Emergency Plan in place and the persons responsible must be contacted in the event of any significant spillage or other such incident. 

9.11	The contractor shall report the discovery of deleterious materials, for example; asbestos, fuel oils, etc. The contractor should take immediate action in accordance with their procedures, to prevent further contact with the deleterious material. All hazardous discoveries shall be entered into the method statements for the relevant project.  Attention must also be drawn to any specific Client or Statutory Authority requirements, which may detail actions to be taken. 
 



[bookmark: _Toc202365984]10. Contamination Management Response Plan

10.1	The following good practice measures are recommended in regard to contamination management.

[bookmark: _Toc202365985]Recommendations

10.2	In order to manage any potential effects of land contamination, the following measures should be undertaken:

•	A piling risk assessment should be undertaken prior to piling work in accordance with the Environment agency guidance on ‘piling and penetrative ground improvement methods on land affected by contamination: Guidance on pollution prevention’; and,
•	If during the development works, new contamination or risks are encountered, works should cease and BMBC should be notified. 
10.3	It is recommended that the contractor put together a response plan which should provide details of how the construction site will be managed to reduce the likelihood of significant pollution such as contamination through oils and fuels.  These measures will include:

•	The Constructor’s main compound will be located on hardstanding areas; 
•	Construction materials and/or waste will be safely stored within either bunded or hard surfaced areas. Bunded storage areas will be located within the constructor’s compound and will be provided for the duration of the works; and,
•	Construction materials or plant will not be stored in any areas which are likely to be at immediate risk of flooding.

10.4	In order to protect surface water drainage, the following mitigation measures should be adopted by the contractor.

•	Construction materials should be safely stored within either bunded or hard surfaced areas as far away from drainage channels as possible; 
•	Any suspected soil/groundwater contamination encountered, not previously identified during investigation works, shall immediately be reported to BMBC and the EA;
•	Regular visual inspections and monitoring shall be undertaken during the construction phase to provide an early indication of any potential contamination releases to controlled waters;
•	Pollution prevention equipment will be kept in the construction area and procedures for use put in place;
•	The Contractor will be required to keep sufficient spill kits on site at all times so that one can be deployed to any part of the construction site within 15 minutes;
•	Construction vehicles will only be active when required and will be regularly maintained to reduce the risk of leakage or spillage. Maintenance work will be carried out off-site or on plant nappies of sufficient capacity to prevent spillage of fuel and oil;
•	Provision will be made to remove any suspended sediments in surface water runoff during excavation and construction works before entering any off-site drainage system; and,
•	All foul and surface water drains will be bunded prior to the start of works.




[bookmark: _Toc202365986]11.0 Waste Management

11.1	The following good practice measures are recommended in regard to waste management.

[bookmark: _Toc202365987]Recommendations

11.2	A site waste management plan (SWMP) will be put in place prior to construction commencing. These should encompass proposals for the control of pollution, together with emergency response plans. The contractor will be required to observe and adhere to relevant legislation and guidelines.

11.3	A Construction Waste Management Strategy should be developed. The generation of construction waste should, as the first priority, be avoided wherever practicable. It is anticipated that spare/waste hardcore/concrete will be crushed into aggregate and reused and spare metal will be recycled. Any remaining materials will be sent to a waste transfer station to recycle, and where this is not possible, will be sent to landfill. Wherever practical, uncontaminated spoil will reused on site for backfill and the regrading of excavations.

11.4	Any waste sent for disposal should be directed to sites which hold valid waste management licenses issued by the EA and which are authorised to accept the type and quantity of waste. Transport of wastes should be minimised by the selection of local disposal sites where available. All contractors used for transport of waste should be registered and licensed haulage contractors following ‘Duty of Care’. No disposal of waste by dumping or open burning should be permitted on site. All waste should be subject to controlled collection and storage on site.
 



[bookmark: _Toc202365988]12.0 Temporary Lighting

12.1	The following good practice measures are recommended in regard to construction lighting.

[bookmark: _Toc202365989]Recommendations

12.2	The construction works will generally be carried out within daylight hours within the permitted working hours; as such the requirement for temporary construction lighting should be limited by this as far as is practicable.

12.3	If, however, there are occasions where temporary lighting is required for occasional night time working or during the darker winter months the following recommendations are made:
•	The use of construction lighting outside normal working hours should be limited and kept to the minimum necessary for workforce, public safety and/or security;
•	No artificial lighting should be placed in locations where it will cause light spillage on habitat corridors which are likely to be used by wildlife; 
•	Any temporary lighting used should be installed such that illumination is minimised and directional so that it is focussed on the specific location/s where it is required; and,
•	Any temporary lighting should be switched off at all times when not required

Appendix A
[image: ]
image1.png




image2.png




image3.png
I Shelter

PONTEF| RACT ROAD
S _ 451m

River Dearne Footbridges
Indicative Compound Layout

letropolitan Borough Council
ighways & Engineering





