STATEMENT OF CONSTRUCTION PRACTICE – LAND AT LOW VALLEY FARM, PITT STREET, DARFIELD, BARNSLEY S73 9PY
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1. INTRODUCTION
This construction method statement has been prepared to cover the residential development of 100 dwelling houses at Land at Low Valley Farm, Pitt Street, Darfield, Barnsley S73 9PY. The development includes associated estate roads, parking areas, public open space and landscaping. This statement has been prepared in respect of conditions 9, 10 and 23 on the Outline Planning Permission Ref 2019/1117.
[bookmark: _GoBack]The relevant conditions are as follows:
Condition 9
Prior to any construction being undertaken the applicant shall submit to the LPA, for approval, a dust management plan which details how dust will be controlled during the construction stages of the development. Once approved the applicant shall strictly adhere to the dust management plan. 
Condition 10
Prior to commencement of development details of dust suppression measures as required
shall be submitted to and approved in writing by the LPA. The approved details shall be put
in place from the start of construction period and shall be adhered to for the duration of the constriction period. 

Condition 23
No development shall take place, including any works of demolition, until a Construction
Method Statement has been submitted to, and approved in writing by, the Local Planning
Authority. The approved statement shall be adhered to throughout the construction period.
The statement shall provide for:

i. The parking of vehicles of site operatives and visitors
ii. Means of access for construction traffic
iii. Loading and unloading of plant and materials
iv. Storage of plant and materials used in constructing the development
v. Measures to prevent mud/debris being deposited on the public highway. 







2. CONSTRUCTION MANAGEMENT PLAN
The proposed Site Execution Plan accompanying this report indicates our proposals for the build route of the site and traffic control measures. In addition, the following items are indicated on the plan and will be installed and managed for the duration of the work on site:
· Position of site compound inclusive of car parking and Welfare facilities
· Access to site compound and throughout site
· Position of site storage and loading areas
· Temporary sales area (including show homes, parking and sales center
· Construction build route/phases of build

3. MEASURES TO PREVENT MUD, GRIT & DIRT LEAVING SITE
The main access of the site connects directly to Pitt Street therefore cleanliness of vehicles and plant travelling between the site and the main road is an important consideration.
This means that action needs to be taken to prevent mud or other debris from leaving the construction site and getting onto the highway. In this instance several measures are being implemented by the developer.
Firstly, road signage erected for the duration of the construction period will be placed either side of the site entrance. The signs will be standard construction warning signage reading ‘Slippery Road’ with ‘Mud on the Road’ sub plate.
A power washing area will be installed next to the site car park so that vehicles leaving the site that require it can clean their tyres and chassis to wash off mud and debris before they exit. Similarly, a power washing area will be installed on the main site road near the site entrance so that other construction vehicles exiting can also be cleaned down before entering the public highway. 
Lastly a road sweeper vehicle will be employed to visit site and clean the site roads each day to prevent a build-up of mud, grit and dirt. This will take place every afternoon prior to the close of site and will also be on call as necessary through each day should there be a need for its services. The site manager will monitor this situation as part of their daily duties and request measures as necessary.
As noted within the submitted site investigation and remediation reports this particular site contains no contaminated land within the developable area thus there is no requirement to remove contaminated land from the site. This greatly reduces the risk of mud and debris being deposited onto the public highways.
Similarly, top soil is to be stripped and stored in safe areas within the site ready to be reused in gardens and landscape areas. Any surplus will be removed by specialist haulage vehicles in accordance with the above statement.
The strip, remodeling and storage of all soil will be wholly retained within the site including the plant conducting the works ensuring minimal vehicular movement to and from the site.
4. MEASURES TO CONTROL EMISSIONS OF DUST & DIRT
The responsible site manager (to be appointed) will ultimately be responsible for dust suppression on the site. Roles and responsibilities are clearly defined within the Barratt Group Occupational Safety, Health & Environmental Management System. A copy of the roles and responsibilities of the Site Manager accompany this statement.
Also accompanying this report is a brief Environmental Policy Statement outlining the group’s vision on environmental issues.
All our Site Managers attend the SMSTS training course on site safety. This course concentrates on Health and Safety which includes the health and safety of the workforce. Part of this is protecting the workforce against environmental impacts, one of with is fugitive dust.
Dust emissions during the construction of buildings or roads are associated with land clearing, drilling and blasting, ground excavation, and cut and fill operations (i.e., earth moving). Dust emissions can vary substantially from day to day, depending on the level of activity, the specific operations, and the prevailing meteorological conditions. A significant amount of the dust emissions results from construction vehicle traffic over temporary roads at construction sites. Dust emissions from residential construction are a function of the total acres of land disturbed and the volume of soil excavated. The volume of soil excavated also varies by type of structure under construction.
Dust suppression is not required in the wetter months of the year. In the drier month’s water will be used to suppress dust where practical. The site manager will be present during all working hours to manage the activity of dust suppression. Vehicle movements will be kept to a minimum.
There are no monitoring and auditing procedures for dust. If dust appears from unidentified sources, the site team will suppress the dust where possible. Safety, Health & Environmental Briefings (SHEB’s) will be provided to site operatives at least monthly and should reflect the actual work being undertaken on site. Records must be maintained of the briefings. All operatives/visitors on site receive a Barratt Group Induction prior to commencing work on site. Environmental Incidents and complaints should be recorded in the incident book on site and records forwarded to the divisional office and Group SHE department as required. Complaints should be dealt with locally by the Division and confirmation of action provided on or attached to the incident report form.
Documentation must be provided for work activities, which is reflective of the work actually being undertaken. The type of control documentation required should be detailed in the Construction Phase Safety, Health and Environmental Plan.
We know what activities create dust and will suppress it. If dust appears from unidentified, unforeseen sources, the site team will suppress the dust where possible.
5. REDUCING NOISE & VIBRATION DURING CONSTRUCTION WORKS
Noisy work is one of the main sources of nuisance from a construction site. The control of noise from this Development will be carried out to mitigate the effects to employees and contractors working onsite and the local residents.
The method of undertaking the work will be completed using the quietest method possible. Wherever practicable all activity will be restricted to below 85dBls
This will be achieved on site by following the HSE guidance on controlling noise at work and by complying with the Control of Noise at Work Regulations 2005.
The noisy element of most construction projects are substructure and superstructure. The methods of Construction will consider the creation of noise and, where reasonably practicable, the method used will be the quietest solutions possible taking into account economic and environmental constraints.
The following actions will be taken to reduce the noise produced on site:

· All machines will be maintained in accordance with manufacturer’s instructions to ensure they operate at their lowest noise levels.

· All generators to be turned off outside of approved working hours. Wherever practicable generators, large drills and breakers will be situated facing away from noise sensitive areas and preferably within the earmarked construction compound areas. All vehicles and mechanical plant used for the purpose of the Works shall be fitted with effective exhaust silencers and shall be maintained in good and efficient working order.
· All compressors shall be “sound reduced” models fitted with properly lined and sealed acoustic covers which shall be kept closed whenever the machines are in use and all ancillary pneumatic percussive tools shall be fitted with mufflers or silencers of the type recommended by the Manufacturers. Special attention should be given to the use and maintenance of sound reduction equipment fitted to power tools and machines.
· Machines in intermittent use shall be shut down in the intervening period between work or throttled down to a minimum.
· Avoid the unloading and loading of equipment and materials between 07.30am and 08.00am within 100 metres of any residential properties.
· Electrically powered equipment should be used in preference to that powered by other sources where reasonably possible.
· Within 100 metres of residential properties no Contractor shall use any air compressor, Pneumatic drill or percussive equipment before 8.00am on a weekday.
· Noise Sensitive areas e.g. Public areas or areas where wildlife is present & occupied plots will be respected and evaluated in accordance with the construction phasing of the development and assessed to ensure noise is kept to below the required levels.
6. HOURS OF WORK (INCLUDING DELIVERIES TO SITE)
The normal working hours within the Site shall be Monday to Friday between 8.00a.m. and 6.00p.m. and Saturday between 9.00 a.m. and 1.00 p.m. with no working on Sunday or public holidays.
Exceptionally, consent for work outside these hours may be given after any necessary consultation. 14 days’ notice is required from the contractor to the L.A Noise levels scheduled for periods outside the normal working hours will only be permitted when consent has been given to exceptional working by the local authority.
7. AVAILABILITY OF STATEMENT
This information will be made available to the public upon request to the Barratt Homes Head Office and also within the site manager’s compound on site throughout the duration of the development.
The construction management plan will be displayed in poster format at large scale within the site compound area so that it is visible by all visitors on first arrival to site.
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