Floodlight Proposal
Four 18m floodlight posts are required in the positions identified on the plan in order to illuminate the whole of the recreation ground and sports field.

The Latest technology in LED Floodlights will be installed. These are more environmentally friendly as they produce less light pollution and are much cheaper to run and maintain than traditional metal halide floodlights. With the floodlights being on 18m posts they will be angled downward throwing the light downwards onto the pitch rather than horizontally. This will remove the potential for any of the floodlights to be an issue in the immediate vicinity of the pitch.
The cost of using the floodlights has been calculated to be approximately £2.20 per hour. 
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The average illuminance provided by the installation of 3 1500w LED lights on each post is 200lux. 
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Plan of Recreation Ground and Sport Field showing the proposed location of the Floodlights
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LIGHTING EQUIPMENT
42 18m Masts Each Carrying the Following AAA-Lux LED Floodiights.
repsrrt "1SSOW Floockoht

2XWS270, 1550W Floodight

HORIZONTAL ILLUMINANCE LEVELS
Specifed level
‘Average Infial Hoizontal uminance (EN.m: 2221

ntained Horizonta urinance (Enm): 2001
u Ratio (E.min| E.av):0.60
Uniformity Rato (E.min € Max): 025

g0 nfialHorizonta Iuminance (EN.m): 259
‘Avorago Maintained Hoizontal Ihuminance (Eh.m):
Uniformily Rato (E.min, € avy: 0.62
Uniformity Rato (E.min € Max): 038

fare Rating: GRma

(Grd ntervals (Footbal Pich) - 88 Peint
ontours Vakes 50, 26,105 8.2 Lux

Maintenance Factor: 09
Based Upon:

- Luminaires deprociaton due 1o it
- Modium Polliion

- Pro-soason cleaning of odights

Notes: Dimensions and Pilch Sizes have boon taken from a customer suppled Imag
mensions shoukd be chacked and confimed on sAe pro 1o lacing an order wh A

‘Scheme develop based upon a flat and open area, where shadowing rom bulding,
auipment have not been taken info consideraion.

0607
26/09/2019

@~ zv e

]























Floodlight





Floodlight





Recreation Ground and Sports Field 





Floodlight





Floodlight





Pavilion








