Further information received from the applicant/agent for application 2024/0430
Amended Bat Report submitted removing reference to removal of the building 
Available to view on Planning Explorer – saved to amended plans 
Queries regarding floor levels 
‘The ground level is to remain unchanged. The finished floor will be higher than the existing floor as recommended by the flood risk assessment. The proposed ridge height is slightly lower than existing, and this is shown on the attached drawing. It is not clear why there is any question that the building footprint, other than the small entrance porch, will remain unchanged.
Please compare the proposed plans with the submitted survey.’ - Rev D saved to amended plans. 
Fencing around the site 
The applicant has confirmed that this is:-
‘Just temporary Herras fencing which will be taken down when renovation completed’
Flood Risk Assessment Additional Comments 
My FRA clearly states that:
Main River
4.2         The nearest EA Main River to the site is the Cawthorne Dyke approximately 3.30km to the north east of the site. Cawthorn Dyke then flows for approximately 300m east into the River Dearne, another Main River.
Ordinary Watercourses
4.3         An ordinary watercourses is located approximately 14m to the north of the site. This watercourse flows west to east for approximately 370m where it joins the Silkstone Beck, another ordinary watercourse. 
4.4         Silkstone beck then flows approximately 2.50km north where it joins the ordinary watercourse section of the Cawthorn Dyke.
I have not said the potential flooding is from Silkstone Beck!!
The FRA recommends that:
5.4         The floor level will be raised to 89.50m AOD, 600mm above existing ground level. 
I understand that although I have recommended raising the floor level that will be internally in the existing building so there is no increase in the footprint or loss of floodplain storage.
Roy Lobley Consulting                                             

