

Phase 1 Trip Generation
The final mix of development must not result in greater than 64 and 63 two way vehicle trips in the weekday AM peak hour (0800 to 0900) and the weekday PM peak hour (1700 to 1800) respectively unless otherwise agreed in writing by the planning authority. 
The total number of trips will be calculated according to the formula as set out below. The development shall then be undertaken in accordance with the approved details.
	
A x 0.538   shall be equal or less than 64 in the weekday AM peak 
  100



AND
	
A x 0.536   shall be equal or less than 64 in the weekday AM peak 
  100



Where A = the Gross Floor Area of development in square metres.
Phase 2 Trip Generation
The final mix of development must not result in greater than 24 and 25 two way vehicle trips in the weekday AM peak hour (0800 to 0900) and the weekday PM peak hour (1700 to 1800) respectively unless otherwise agreed in writing by the planning authority. 
The total number of trips will be calculated according to the formula as set out below. The development shall then be undertaken in accordance with the approved details.
	
A x 0.538   shall be equal or less than 24 in the weekday AM peak 
  100



AND
	
A x 0.536   shall be equal or less than 25 in the weekday AM peak 
  100



Where A = the Gross Floor Area of development in square metres
Total Trip Generation
The total mix of development (All Phases) must not result in greater than 88 and 88 two way vehicle trips in the weekday AM peak hour (0800 to 0900) and the weekday PM peak hour (1700 to 1800) respectively unless otherwise agreed in writing by the planning authority. 
The total number of trips will be calculated according to the formula as set out below. The development shall then be undertaken in accordance with the approved details.
	
A x 0.536   shall be equal or less than 88 in either the weekday AM peak or the weekday PM Peak
  100



Where A = the Gross Floor Area of development in square metres.

