Design & Access Statement
Site Address


185-187 Sheffield Road, Barnsley. 
To Convert G.F. into a Training Café for use by the Public but to train staff as well
The brief was to convert classrooms to the g.f. into an open space to be used as a café with a kitchen facility built in.
The elevations will be unchanged from the current aspects both to the front and to the rear.
Physical Context

The surrounding area is made up of similar Victorian terraced houses
Most buildings in this area appear to be aprox 100 years old.

The surrounding area is predominately residential with adjacent buildings to this one already converted into offices.
The access route to the property is gained via a 1m wide path running upto the house as shown on the block plan.
The proposed disabled access will be via the rear door
The Site

Is currently used as a teaching/educational classrooms for the building trade operated by BCB.
The site is a level site without gradient
The boundaries have no vegetation bushes trees or otherwise.
Social Context

There is no loss of existing buildings either residential or commercial on this site.

Local services would not be affected from many points of view, the sewers would be connected into main drains.

Public transport would not be affected from this development if anything it would help bolster up local transport by putting more people on the busses making it a more profitable venture. A local service runs on a regular basis and travels into Barnsley.
Economic Context

There will be jobs created from this development other than those by builders to operate this facility.

The neighbours have been consulted i.e BCB.

No amenity groups have been consulted.

Evaluation

There are no constraints on the development that we are aware of from a physical/social/economic context.
Design of the Scheme

The design of the exterior will be unaffected and will remain exactly as it is now.. 
Access

Access is directly from Sheffild Road pavement for pedestrians and for disabled a level threshold is available to the rear door.
The house is situated in a prime position with a bus service passing by every 15mins.
Surface water will be disposed of into a soakaway
Foul drainage will be piped into existing main drain.
The principal entrance to the dwelling to have a level threshold with a path at least 1m wide upto it from the path to the rear constructed of a hard material i.e. block paving, concrete, tarmac not loose chippings or pebbles for wheelchair access.

All openings and doors must have a min opening width of 840mm or 2’9” doors again for wheelchair access.

Radiators should not be positioned opposite doors and electrical sockets and light switches are to be positioned between 450 & 1200mm above floor level.

The toilet should have an outward opening door

As there is no flood risk floor levels can be set at a standard 150mm above ground level.

Scale

The scale of the proposed work is soley conversion, the top two floors will remain as classrooms with access via a 2nd rear door.
Appearance

Unchanged from present 
Layout
The position of this proposed cafe is situated close to main arterial routes serviced by a regular bus service .

The surrounding area is of a level topography making it easy for the elderly and disabled to get about.

The owners will be fitting this cafe out with security features such as 5 lever locks or better to doors, window locks, a burgalar alarm system and exterior lighting activated by movement and by low light.

This concludes the design and access statement

