T1 Sycamore
-Dismantle and remove to ground level 

T2 Sycamore 
-Crown lift all branches to around 3.5 metres
-Crown reduce by around 1 metre to reduce the wind loading on the tree which will be increased with the removal of T1
[bookmark: _GoBack]-20% thin of the remaining canopy to allow more light through to the property and to facilitate vehicular access
