Customer Extra car charge options
1. Simple external 13amp waterproof socket nr car park space with dedicated circuit and fused isolation spur £138.00
2. Pre-wire for future car charge point (cable left unterminated within distribution board and external IP box £63.00
3. 13amp (2Kw) 3 pin socket Rolec wall pod (EVWP0020) with PEN isolation device (EVIN0050) adjacent the distribution board. £306.00
4. 16amp (3.3Kw) type 2 Rolec wall pod (EVWP2010) with PEN isolation device (EVIN0050) adjacent the distribution board. £656.00
5. 32amp (7Kw) Fast Charge type 2 Rolec wall pod (EVWP2020) with PEN isolation device (EVIN0060) adjacent the distribution board £693.00
Items 3, 4  and 5 must be either installed with an earth rod in the drive which is not practicable as it has to be 5mtrs from the house and boundary or with A separate means of disconnection from the house supply should a fault occur with the car internal circuit. We would therefore fit the PEN unit which eliminates the need for the earth rod. This is needed to conform with the current BS7671 regulations, but these may be changed early 2021 to negate the need for additional protection. If this occurs, we will let you know as soon as we know.


