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PLANNING CONSULTATION RESPONSE
	Application No
	2026/0108

	Proposal
	Erection of 4 padel courts with a covering structure, installation of a football pitch and erection of a new associated building to include changing facilities and cafe/social areas.



	Address
	Burntwood Sports and Leisure Centre, Common Road, Brierley, Barnsley S72 9ET


	Date of Consultation Reply 
	03/06/2026

	Consultee
	Highways Development Control



	Consultation Assessment and Justification

	Many thanks for consulting Highways Development Control in respect of this planning application.

The proposed development involves upgrading the existing Burntwood Sports & Leisure Centre by adding padel courts, a 3G football pitch, and a new clubhouse with café and changing facilities. Vehicle access will remain as existing, continuing to use the current junction from Common Road, along with the established internal access routes car parks. 

Following my initial consultation, a Highways Statement was submitted to address questions raised in respect of trip generation and car parking availability.

Currently, the site generates approximately 134 two way trips during the morning peak and 178 two way trips during the evening peak, based on observed data and in order to understand the potential trip generation for the proposed changes, trip rates from the TRICS database have been applied to the café element, alongside assumptions for use associated with the sports facilities.

The resultant predicted trip generation is circa 54 additional trips in the AM peak and 37 in the PM peak. However, this approach assumes that each component operates independently and generates entirely new trips. In reality, many of these journeys are likely to already form part of existing travel patterns, as a proportion of users are expected to come from the current membership base. As such, this represents a robust scenario, and actual trip generation is expected to be less and involve shared and linked journeys.

With regards parking, existing demand has been assessed using ANPR survey data, which provides a reliable picture of how the car park operates throughout the day. This identified a peak accumulation of 153 parked vehicles between 18:00 and 19:00 and with a total of 203 spaces available on site, there is clear spare capacity even at the busiest time. 

However, assuming that the padel courts, football pitch and café all operate at full capacity simultaneously and independently an additional demand of 64 parking spaces could arise, resulting in a total requirement of approximately 217 spaces—exceeding the 203 spaces available on site by 14. However, this scenario is unlikely to occur in practice. It assumes full and simultaneous use of all facilities and that all trips are new, which does not reflect how the site will likely function. Demand will be staggered throughout the day, with the café more active during daytime periods and sports uses peaking later. Accordingly, this position could be viewed as a theoretical maximum rather than a realistic outcome.

Overall, the assessment indicates that any increase in trip generation will be modest. Furthermore whilst car parking capacity may appear tight under extreme assumptions, the evidence suggests that the existing provision of 203 parking spaces is sufficient in practice. Therefore, the development is unlikely to result in overspill parking or a material impact on the surrounding highway network.

As such, there are no objections from a Highways perspective, subject to the conditions and informatives indicated below. 


	NO OBJECTION*
	Defer for amends/further information*
	OBJECT*

	*Delete as applicable

	Consultation Suggested Conditions:

All on-site vehicular areas shall be hard surfaced, laid out and drained in an approved manner prior to the development being brought into use, to prevent mud/debris from being deposited on the public highway to the detriment of road safety.

The parking/manoeuvring facilities indicated on the approved plan shall be provided prior to the development being brought into use and shall be retained for that sole purpose at all times, in the interests of road safety.

Vehicular and pedestrian gradients within the site shall not exceed 1:12 to ensure safe and adequate access.


	Consultation Informative(s):


The contractor shall ensure that no vehicle leaving the development hereby permitted enter the public highway unless its wheels and chassis are clean. It should be noted that to deposit mud and debris on the public highway is an offence under provisions of the Highways Act 1980.




	Planning Obligations required:
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