[image: image1.wmf]
TOLENT CONSTRUCTION LIMITED

SITE WASTE MANAGEMENT PLAN

FOR THE

BURLEIGH MEDICAL CENTRE

AT

BURLEIGH STREET, BARNSLEY

Tolent Construction Limited

Cleveland House

Dukes Court

Teesside Industrial Estate

Thornaby

Stockton on Tees

TS17 9LT

Tel No:
 01642 308005

Fax No: 01642 765953

List of Contents

Introduction/Brief Project Description





1.0

Project Responsibilities







2.0

Site Waste Identification







3.0

Details of Waste Removal Contractors





4.0

Details of Waste Transfer Station





5.0

Site Material Handling Details






6.0

Training Requirements







7.0

Waste Measurement







8.0

Monitoring/Review Arrangements





9.0

Waste Hierarchy Flow Diagram






10.0

1.0
Introduction/Brief Project Description

1.1
Introduction

This site waste management plan provides a structure for waste delivery and disposal at all stages during the construction of this project and all projects with a value of over £300,000.00.

The aim of this plan is to help protect the environment by managing materials and waste more efficiently, which also should assist in reducing costs.

In terms of this plan the definition of waste is any material that is not used within the works and has been removed from site.

1.2
Brief Project Description

The Project comprises of the construction of a 2-storey health centre. The foundations are pad type with ground beams, Metal Deck with screed, steel frame, external cladding skin and glazing with associated drainage and hard and soft landscaping.

1.3
Client Details


Dr Samanth Chikthimmah


Park Grove Burleigh Limited 


drchikthimmah@gmail.com

07825836949

2.0
Project Responsibilities

2.1
Person in control of the site is:  Jeremy Marley

2.2 Person responsible for the implementation of the plan is:  Jeremy Marley

3.0
Site Waste Identification

List main types of site waste, resulting from the construction operations: (include contaminated ground if applicable and type of contamination).

Estimates Only

	Waste Type
	EWC Code
	Target Quantity (Tonnes)
	Contain Type Skip/Bin etc
	% Recycled or Re-used



	Active

(mixed construction and demolition waste)


	17-09-04
	70
	Skip/Wagon
	100% recycled off site

	Inert

(bricks, concrete, tiles, ceramics,clay)


	17-01-07
	15
	Skip/Wagon
	100% recycled off site

	Compactable

(mixed municipal waste)


	20-03-01
	20
	Skip/Wagon
	90% recycled off site

	Timber


	17-02-01
	5
	Skip/Wagon
	50% re-used

50% recycled off site

	Metal


	17-04-07
	6
	Skip/Wagon
	100% recycled off site

	Plasterboard


	17-08-02
	10
	Skip/Wagon
	100% recycled off site

	Asbestos + Asbestos Cement Materials


	17.06.01
	0
	
	

	Glass


	19.05.04
	0
	Skip/Wagon
	

	Reduced Level Dig/Materials


	17.05.04
	100
	Wagon
	100% re-used

	Tarmac


	17.03.02
	0
	
	


4.0
Details of Waste Removal Contractors

To include name, contact name, address and waste carriers, etc. details, telephone number.

BWS LTD

263 Whitehall Road

Leeds

LS12 6ER

mail@bwskiphire.co.uk
5.0
Details of Waste Transfer Station


To include name, address, waste license details, telephone number.

BWS Waste Management

263 Whitehall Road, Leeds, LS12 6ER

Waste license : CBDU65874

0113 2311470

6.0
Site Material Handling Details

6.1
Outline the methods of material handling to be used on site, to reduce the risk of damage etc, ie telehandler, masted forklist, crane, hoist etc.


Excavators with site dumpers together with forklifts will be used for general transport from store area to place of work.


Cranes will be used to deliver materials to roof level.

7.0
Training Requirements

7.1
Site waste management and environmental management is explained to all persons new to the site during the induction.  Any additional specific training requirements is/can be arranged via the Company Safety Department.

8.0 Waste Management


Estimated the amount of waste likely to be produced on site, so the best method of removal can be adopted.  It is advised that the detailed design should be progressed well ahead of construction operations to prevent incorrect ordering of materials.  Where possible, avoid designs that need major on site cutting of materials, as this increases the production of site waste.  Request materials to be delivered banded, rather than boxed, shrink wrapped etc.

8.1
Wherever possible separate skips will be used to segregate waste material.

9.0 Monitoring/Reviewing Arrangements


This plan shall be reviewed every four weeks by the Site Manager/visiting Safety Managers.


Results of the review shall be documented and copies sent to the Contracts Manager.

10.0
View Hierarchy Flow Diagram











ELIMINATE





Avoid producing waste








DISPOSE





Dispose of what is left in a responsible way








RECYCLE





Recycle what you can only after you have re-used it








RE-USE





Use items as many times as possible








REDUCE





Minimise the amount of waste we produce








