Location

The property is located along station road and is within the Brierley Conservation area and is a back land existing development, and is entered between two rows of terrace properties. The new structure will not be visible from a public highway.

Existing Structures

There are 4 small individual timber structures with a mixtures of roof types and finishes, they comprise of corrugated felt sheeting, felt and cement fibre slates of lean to and close couple type roof structures. They house 2 vintage tractors, a horse carriage and stores for livestock. They are located at the side of the existing domestic residence and overlook the community centre and back onto the boundary line between the applicants land and the adjoining owners (approx 1.5m from the boundary).
Wall construction is of a mixture of timber slatted boarding and stramite board, varying in height from approximately 1.9m to 2.3 – 2.5m to there apexes. 

The sizes of the sheds are as follows, 2 at 1.5 x 1.8m, 1 at 3 x 3.5m and 1 at 2.4 x 3.5m all sizes are approximate. 
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Picture Showing Side View of Existing Sheds
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Other side View of Shed
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Front View of Sheds

New Stable Block

The proposed construction of the new stable block is due to the deterioration of the existing timber stable block within the field. The construction of the block will comprise of matching brickwork and natural slates to the roof with 3 subdivisions to house both horses and the vintage tractor. The new stable block cannot be seen from the public highway. It can only be seen from the Village club and the properties to the rear of the applicant. It will help to improve the character of the area by blending into the surrounding by the use of the matching brickwork of the house and the use of natural welsh slate for the roof which also matches the house roof.
