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METHOD STATEMENT

PROCESS
The erection and maintenance of security hoarding
METHOD
1. Thoroughly read through risk assessment and be aware of any site specific instructions that need to be complied with.
2. A small security fencing compound will be formed in order to maintain access in front of the building and allow deliveries to offload materials on regular basis.
3.Security hoarding to be enclosed in a blue netting to enclose and maintain minimal activities been seen behind.
4. Any deliveries or construction traffic coming to site must sign in and report to the Site Foreman. 
[bookmark: _GoBack]5. Deliveries will follow the correct manoeuver procedure using the banksman on site.
MEANS OF SAFE ACCESS
Access to the working area will be via the front/rear doors of the premises.

PERSONAL AND RESPIRATORY PROTECTIVE EQUIPMENT
Tradesmen will be provided with necessary PPE and RPE by Whitshaw Builders Ltd. including ear
defenders, protective gloves, gauntlets, eye protection, hard hat, safety boots, high
visibility vest, knee pads and respirator/dust mask. Tradesmen will wear high visibility vest and safety boots at all times on site. Specific PPE requirements are detailed in the method statement above.

Tradesmen will assess the need for using additional items for each part of the operation and have
been trained to do so. Any mandatory site safety requirements will be complied with.
ELECTRICAL EQUIPMENT
110 volt equipment only will be used. This is to be visually inspected for damage by tradesmen at
the commencement of each working day and to be within test date.
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