
DESIGN & ACCESS GUIDE

ERECTION OF A NEW AGRICULTURAL BARN AND STABLES 
LAND OFF COMMON LANE, BRIERLEY, BARNSLEY, SOUTH YORKSHIRE.
Development proposals

(Please refer to current drawings CONN-001 to 004)
The development consists of:
· 2 Agricultural buildings consisting of stables and a storage barn
The site at the above address is located approximately 4.87miles from Barnsley Town Centre. The site is situated to the immediate south of Common Lane and is approximately 10 acres or 4.05 hectares in area. 

This document will set out the design route to this planning application; namely the development of two agricultural buildings for the stabling of horses and the storage of machinery and hay.
Each building has a gross internal floor area of approximately 97.5 sqm making a total of 195sqm for the pair. Both buildings will be identical and are to be built off a stone base with the upper walls consisting of timber clad walls with a metal standing seam roof similar to the picture below. A winding single track will lead across the field to the entrances of both buildings. In addition a perimeter fence will be erected around the site.
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ACCESS

The site entrance will be to the North West corner of the site off Common Road as indicated on dwg no CONN-001 and CONN-002. The visibility is considered acceptable and the access will provide the following:
· The gate to protect the site and barns from intruders will be positioned 12m from the carriageway in order to allow a vehicle to stand off the road whilst the gate is opened

· The gate will open inward

· The first 12m will be paved in tarmac or concrete.

· The access shall have dropped kerbs must be provided to restrain the existing carriageway
· The entrance and access are to be single track

DESIGN
The stables are required to house the client’s horses, of which he will have a maximum of 6 for domestic use only. The hay is to be grown and processed on site therefore the barn is required to safely house the equipment required to process the hay, including a tractor and a bailing machine. This barn is also required for storage in order to ensure the hay can dry in a safe location on site, therefore reducing transport requirements and in turn pollution. This ensures that all processes can be carried out on site creating a more sustainable agricultural development for this green belt area.
In addition a number of changes have been made to the scheme, which are a significant departure from the previously refused scheme. These are:
· The position of the barns is now close to the boundary with the existing agricultural buildings on the adjacent site to the North West. The buildings register as a more cohesive cluster with the adjoining buildings and are far less exposed and visually intrusive than they were on the previous scheme.

· The buildings have been reduced in size from approximately 110 square metres (sqm) to 97.5 sqm of internal floor area. We wish to provide accommodation for 6 horses and the minimum recommended size for a standard horse pen as recommended by the British Horse Society is approximately 3.7m by 3.1m (12ft x 10ft) although a slightly larger 3.7m x 3.7m (12ft x 12ft) would be preferable. However the minimum recommended size has been incorporated into the layout in order to keep the size of the stable to a minimum.

· A new site access has been created off Common Road with a track shown leading up to the new barn and stable. This new access is located along a relatively straight section of Common Road and highways have confirmed that the visibility is acceptable.

· The materials for both buildings have been changed to a more acceptable arrangement. They will be built off a stone base with the upper walls consisting of timber clad walls and a metal standing seam roof similar to the picture below. This approach will ensure the continuity and longevity of the buildings.
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