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Application Number 2017/1718
Residential development for up to 85 dwellings with associated infrastructure and access (Outline with All Matters Reserved apart from access)
Former William Freeman Site, Wakefield Road, Mapplewell, Barnsley, S75 6DN


Hannah,

There are proposed drainage details shown on the plans submitted, with the application form describing foul to discharge to “main sewer” and surface water to “main sewer”.
There is a public sewer in the area so foul should be no problem.

[bookmark: _GoBack]I also refer to the Drainage Strategy submitted by Topping Engineers regarding the drainage of this site; the FRA gives a strategy with respect to the drainage of the site, but is short on the final details regarding final method of disposal of surface water 

Whilst I have no objections in principle to the proposals, I think that due to the size of the development and potential impact on the watercourse and to ensure that the outfall is investigated further, full drainage details should be sought early on in any a reserved matters application.  

H4 - No development shall take place unless and until full foul and surface water drainage details, including Yorkshire Water Permission to discharge, have been submitted to and approved in writing by the Local Planning Authority. Thereafter no part of the development shall be occupied or brought into use until the approved scheme has been fully implemented. The scheme shall be retained throughout the life of the development unless otherwise agreed in writing with the Local Planning Authority. @ To ensure the proper drainage of the area

H5 No piped discharge of surface water from the application site shall take place until works to provide a satisfactory outfall for surface water have been completed in accordance with details to be submitted to and approved by the local planning authority before development commences. @ To ensure that the site is properly drained and surface water is not discharged to the foul sewerage system which will prevent overloading.

H6 - No development approved by this permission shall be commenced until a scheme for the provision and implementation of a surface water run-off limitation into the watercourse has been submitted to and approved in writing by the Local Planning Authority. The scheme shall be implemented in accordance with an approved programme and details. @ To prevent the increased risk of flooding.


Advisory Notes

If the developer is to make discharge flows to the existing watercourse he must gain the written agreement of the Land Drainage Authority to discharge flows at an agreed rate – Contact Wayne Atkins (01226 772182)

If the developer is to carry out works within or in the proximity of any watercourse he must gain the relevant permissions from the Lead Local Flood Authority – Contact Wayne Atkins (01226 772182)

Regards



Ian Grayson
Senior Engineer – Drainage and Highways
Network Resilience and Asset Management
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