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1. Introduction & Scope of Works 
INTRODUCTION

	The project comprises  the demolision of the existing garage. Erect ion of a two storey rear extension with single storey extension for utility and garage/workshop. 


SCOPE

The scope of this MS and RA is to detail the way in which trees will be preserved, pruned and or removed to afford the construction of the new extension works
2. Working Areas & Boundaries 
There are 4 designated working/affected areas.
1. Existing garage to be removed to the front left hand side of the property – Surrounded by bushes and shrubbery 
2. New kitchen & utility room/w/c extension to the rear left of the property – Hedges along the adjoining property boundary
3. New garage and double storey extension to the rear and rear left of the property – Shrubbery, bushes,1 No Silver Birch and 2 no conifers in this area.
4. House frontage / front boundary – 2 No established trees (1 Copper Birch & 1 Cherry Blossom)

3. METHOD OF WORKING & REINSTAEMENT
 3.1 Work area No 1 
· Schedule of any tree surgery works (Removal and pruning)

All surrounding bushes and shrubbery to be removed by hand or by mechanical means. 

· Details of tree protection (protective fencing, separation distance from works etc.)

No protection required as no trees or other specified items in the area within +5m
· Specifications of level and surface changes

This area will be levelled and covered with terram or other material to effect the proposed drive extension.
· Trenching methods (how excavation will be carried out without damaging tree roots)

This area will be cleared by pulling the shrubbery/bushes out by hand and digging out roots where required by hand.

· Details of additional tree planting (if any is proposed)

Trees, shrubs or hedging will be placed along the property boundary line where suitable and desired.
· Copies of the site plan and tree survey

Refer appendix A attached site layout drawing

3.2 Work Area No 2
· Schedule of any tree surgery works (Removal and pruning)
Laurel and Ivy Hedge line to be trimmed and removed where necessary

· Details of tree protection (protective fencing, separation distance from works etc.)
No protection measures required as no trees in this area within +5m
· Specifications of level and surface changes
· Trenching methods (how excavation will be carried out without damaging tree roots)
N/A
· Details of additional tree planting (if any is proposed)
N/A

· Copies of the site plan and tree survey

Refer appendix A attached site layout drawing

3.3 Work Area No 3
· Schedule of any tree surgery works (Removal and pruning)
Shrubbery, bushes and 2 no conifers to be removed by hand lopping and chainsaw at the left hand boundary fenceline with tree roots removed by mechanical means wherever required.

The Existing Silver Birch Tree and Conifer (to the rear of the new garage and double storey extension) will remain in place and no pruning is foreseen 
· Details of tree protection (protective fencing, separation distance from works etc.)
Protection will be afforded using suitable de-markation fencing (1m from the existing conifer) to secure shrubs and 1 no Silver Birch and 1 No Conifer in this area. The Silver Birch roots have previously been investigated and found to be 1.3m from the tree trunk and the conifer stands between this and 2m from the proposed foundations
· Specifications of level and surface changes
Surfaces will be levelled soil and excavations for foundations.
· Trenching methods (how excavation will be carried out without damaging tree roots)
Foundation excvtions will be undertaken by mechanical excavator
· Details of additional tree planting (if any is proposed)
N/A
· Copies of the site plan and tree survey

Refer appendix A attached site layout drawing

3.4 Work Area No 4

· Schedule of any tree surgery works (Removal and pruning)
The Cherry Blossom tree will be not be affected oby the works and will remain insitu and un-touched.
The Copper Birch will be pruned to effect the entry of large vehicles and materials onto the property works area. This will be undertaken by pruning using hand loppers and/or chainsaw. Only essential branches will be removed and supervised by the building works supervisor and those removed will be to the maximum height expected (approx 4 metres) of incoming vehicles.
· Details of tree protection (protective fencing, separation distance from works etc.)
N/A

· Specifications of level and surface changes
N/A
· Trenching methods (how excavation will be carried out without damaging tree roots)
No excavation will be undertaken to affect tree roots.
· Details of additional tree planting (if any is proposed)
N/A
· Copies of the site plan and tree survey

Refer appendix A attached site layout drawing.
4.0 General Statement

Whilst the trees, etc have no known TPO’s listed, every attempt will be made to minimise the affect on these that may arise from the ensuing works.
The property is an old one with a well established yet overgrown garden, which will be my wife and my home, so preservation is key for us. For the good of the property and garden we shall plant more trees and shrubs to replace the ones removed wherever possible around the new extension.

Any change to any of the methods contained in this document will be subject to approval with Barnsley District Planning or their representatives consent only.
Appendix 1 General Site Layout Drawing
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