Planning Statement – Worsbrough Mill, Bakery extraction 
Currently there is an issue with the lack of extraction from the bakery situated in Mill Cottage.  This leads to the build-up of steam, flour and dust particles as they are not able to be efficiently removed by the domestic extractor fan fitted in the upper window of the gable end.  Several solutions have been proposed but, following discussions with BMBC’s Senior Conservation Officer, this one is seen to be the only viable option.
The black painted, metal, louvre grille is to be fitted in place of a single pane of glass in a window on the return wall from the gable end of Mill Cottage.  Although Mill Cottage is a Grade II listed building this alteration is totally reversible and will have very limited impact on the building.
The exact location has been chosen so that is on a side elevation of the building with the colour of the grille having been chosen to further minimise its visual impact.
In addition, the existing fan in the gable end window will be removed and replaced with a full pane of glass so making this elevation closer to its original state.


