

	[bookmark: _Toc479151853][bookmark: _Toc479152398]Darley Cliffe Hall, Upper Sheffield Road (west side, off) Barnsley, South Yorkshire. 

A Second WSI (June 2020) to supplement the WSI and the Archaeological ‘Watching Brief’ Record made during investigative works to the Kitchen attached to the north side of Darley Cliffe Hall

	Written Scheme of Investigation for a Structural Watching Brief for proposed Extensions to the Kitchen and lowering of ground levels around the main mansion house                                                                                               Prepared by Peter Thornborrow Historic Buildings and Conservation Consultant, 28th June 2020



Introduction

Summary 
[bookmark: _Toc479151854][bookmark: _Toc479152399]This written scheme of investigation (WSI) has been prepared on behalf of Mark Ludlam. by Historic Building Consultant Peter Thornborrow (PT) in consultation with Buildings Archaeologist Paul Gwilliam HBO (PG) to confirm a programme of historic building recording at Darley Cliffe Hall (hereafter ‘DC’). 
The requirement for a programme of historic building recording, and the preparation of a WSI, was outlined in Condition 3 of the Draft Conditions prepared by BMBC for the Courtyard Extension to be built onto the west side of the Kitchen Wing at DC (see Appendix 1), the application submitted by the architectural practice BPB. This will be prepared in accordance with the Revised Proposals Report outlining the proposed recording methodology submitted to BMBC and SYAS on behalf of the owner Mark Ludlam, Director, for approval by PT, dated 06/03/2020 so as to establish an agreement for the scope of works in advance of the preparation of this WSI.
This proposed programme of works of investigation is in accordance with the detailed guidance provided by SYAS (see Appendix 2). It will be phased in three parts, better detailed in Section 4:  
Part 1 to make drawn and photographic records of the inward facing elevations of the buildings lining the three sides of the stone-flagged courtyard area prior to the construction of a new extension attached on to its west side. 
Part 2 to make photographic records of all the external elevations of Darley Cliffe Hall and its attached buildings on the north side. 
Part 3 for a structural Watching Brief during works of demolition and excavation of the relatively modern extension built on to the north side of the Kitchen wing. 
Each of these phases will form a permanent record in the form of three separate but connected reports as each phase of the development is completed. They will utilise the ‘as existing’ survey drawings that accompanied the application, but annotated and modified adding any relevant architectural features not shown (such as the blocked arched doorway in the west wall of the kitchen, and for these to be accompanied by photographs taken by PG. 
These reports will be linked to and supplement the existing ‘Watching Brief’ report already undertaken as prepared by PG, and submitted to the LPA as part of the current application for a new extension, of the investigative works made in advance of proposed alterations to the interior of the Kitchen, and will form part of a permanent record as a single-archive for deposition with the local authorities museum service in accordance with the requirements of SYAS as outlined in the ‘Model Brief for Archaeological Monitoring (Watching Brief) already referred to above (See Appendix 2).
[bookmark: _Toc479151855][bookmark: _Toc479152400]The Kitchen is a single room contained within a single-storey stone-built small building with a pitched stone-slate covered roof. It is built on to the north side of Darley Cliffe Hall, a Post-Restoration mansion of c.1685 that has a double-pile plan. It is connected to the house by a door in the north wall of its Stair Hall, immediately adjacent to the door to the Cellar. The Kitchen was added on to the building at an uncertain but later date than the original house; in earlier reports (Heritage Statements prepared by PT) this was assumed to have been added in the mid-18th century from stylistic evidence of the king-post roof truss, purlins and rafters. However, recent investigative work suggests that the external walls of the building were subject to major alterations during the second-half of the 20th century and in more recent years as confirmed by the inner walls mostly lined with modern Imperial-sized brickwork, and in the window reveals - visible after the removal of modern Gypsum plaster and plaster board during the investigative works survey. By tradition the original kitchen was believed to be located in the earlier Tudor House attached on to the south side of the Hall, that since c. 1977 has formed a separate property. A Structural Watching Brief was undertaken internally in the Kitchen during stripping-out works involving the removal of plasterboard from off the walls and ceiling, and  the discovery of the original stone flagged floor underneath a modern concrete slab floor that overlaid it and was broken up. As part of the recording work a scaled floorplan was prepared and the flags were carefully numbered as they were taken up prior to storage in original rows and being re-laid in the same position. In addition the original stone fireplace was rediscovered with a tapering hand-made brick flue built against the north gable; this supported the original Georgian date suggestion. Convincing evidence supported the restoration of the original form of the fireplace with three openings with two new stone lintels and jambs based on the surviving kitchen fireplace at Barnsley Council’s Cannon Hall Museum. The restored fireplace should now be photographed and for this to be included with the earlier record.
The Kitchen by virtue of being attached on to the side of DC is a designated heritage asset and therefore is afforded protection under paragraph 197 and 199 of the National Planning Policy Framework NPPF (revised 2018). 
Paragraph 199 states that:
“Local planning authorities should require developers to record and advance understanding of the significance of any heritage assets” 
This document has been produced in accordance with best practice set out by the Chartered Institute for Archaeology (CifA 2014a) and by Historic England (2016a). Further guidance was supplied by BMBC Conservation Officer who requested that ‘a Historic England structural watching brief of …. was undertaken prior to, and during the removal of material’.
Site Description
Darley Cliffe Hall was built as a gentleman’s residence in c.1685, but an early 19th century map shows it situated in an open farmyard. In the last quarter of the 20th century all the larger farm buildings were converted to residences and the smaller building (pigsties and similar) were demolished. At that time the hall was separated off from the two barns and the coach house and was set behind an elegant gated entrance, linked to possibly earlier 19th century walls; the curtilage of the house changed. The former farmyard is now partly turfed with a garden on its north side bounded by a good neat stone wall, with a large gravelled area in front of the east side of the house that is now used for car-parking.  This area is now approached through tall wrought-iron gates (added some time during the period 1980-2000?) designed to provide the look of a grand country-house entrance. The symmetrical entrance front of the Hall is enclosed within a small walled-garden (probably late-17th century and contemporary with the house) that is set before it and enhances its setting. It is approached off an unnamed road on the west side of Sheffield Road, approximately 1 mile from the centre of Barnsley, centred at National Grid Reference SE 35551 04524 (Figure 1). 
[bookmark: _Toc479151857][bookmark: _Toc479152402][bookmark: _Toc479151862][bookmark: _Toc479152407]HISTORICAL AND ARCHAEOLOGICAL BACKGROUND
The kitchen built on the north side of DC is first shown on Spooner’s large-scale map of Barnsley (c.1861), pre-Ordnance Survey. This shows other buildings attached on to the north end of the kitchen (since demolished) set at right-angles to it that extend beyond the building line on the entrance side, and backwards linking to the adjacent barn, that now  forms a separate dwelling. This is significant in that it demonstrates that buildings were attached onto the kitchen wing, dating at least the early 19th century. The foundation of these may be revealed during the final phase of the proposed development, following the demolition of relatively recent buildings (last 50 years), and the excavation for foundations for a new proposed extension in the same area. This confirms the need for a Watching Brief during these works which have not yet been submitted but are nearing completion. They are covered in this WSI so that the programme of recording work is agreed for these future buildings obviating the need for the preparation of another WSI.
Prior Investigations
A detailed Heritage Statement detailing the history of the main house and its architecture was previously submitted to accompany the various submitted applications: for the repair of the lead-flat of DC’s roof, and for alterations to the house (application no. 2019/1297) that was granted LBC - the works currently nearing completion. 
As the present applications are purely concerned with the proposed extensions to be built on to the sides of the kitchen – itself a later ancillary building – it is not considered necessary in this instance to repeat the previous Heritage Statement that is readily available (see below). The Kitchen and its additions are subject to a careful evaluation in para. 1.18 at the end of Part 1B (as revised 11.09.19) of my Heritage Statement for Darley Cliffe Hall, where the long-term aims of the owner to introduce disabled facilities, and the provision of a ground-floor bedroom, is first outlined. Follow this link:
https://wwwapplications.barnsley.gov.uk/PlanningExplorerMVC/Home/FileDownload/67c0a2b3-fb7b-4db4-aad5-04d4dee03ab3?ApplicationNumber=2019%2F1297

AIMS AND OBJECTIVES 
The aim of this WSI is to outline a programme of works to be recorded in a Structural Watching Brief in the area of the Kitchen to cover two proposed new extensions. This accords with recognised good practice to record alterations to historic buildings prior to and during development.
The work aims to record the extent, condition, character and date (as far as possible) of the buildings attached to the kitchen wing and to comment on its historic development which will be detailed in a final report. The results of the recording will be placed within the public domain to inform future research and act as a permanent record of the building made during alteration. 

scOPE OF THE work 
Map Regression 
A map-regression exercise of all Historic large-scale (25” and 6”, but not 1” to the mile) Editions of the Ordnance Survey maps (to include the latest available) should be undertaken; relevant extracts should be copied and included in the final report (see 4.1.21) with a commentary noting any changes in the farmyard around Darley Cliffe Hall, and its curtilage, that differ from Spooner’s earlier map of 1861.  
The Phased Record
0. Phase 1. The Courtyard Extension: As plans and elevation drawings of the building already exist, these will be used as a basis for the final drawn record, but these will be checked and altered accordingly for the final report. The drawings shall be annotated and drawn using the conventions outlined by Historic England. Each of the three external elevations of this courtyard are to be so annotated in the drawn record with a written commentary describing each wall elevation. 
North elevation of the Hall: note should be made particularly of the blocked sash window. This should be carefully drawn at an appropriate scale to show its construction from different pieces of stone. 
[bookmark: _Hlk44180116]Proposed alteration: the side jambs of the window will be dismantled and lowered to form a doorway, requiring the removal of the window sill and the walling below it, but without any additional stonework to the jambs; in this manner the original window surround will be retained but converted to a doorway to form a link between the new courtyard extension area and the existing Dining Room of the Hall. The stonework of this window will be carefully dismantled and rebuilt lower and slightly to the right, so as to better fit with the internal wall panelling of the Dining Room. Internally this will have a jib-door fitted cut-into the wall panelling as a hidden door, but with a separate door on the extension side. This will involve the loss of the internal cupboard (constructed inside the blocked window opening) that will be removed during this programme of work. A detailed drawn and photographic record of this cupboard and the complete internal panelled wall of the Dining Room will be required prior to the commencement of any works of dismantling. The recorder should also be in attendance to record the dismantling of the window prior to its reinstatement as a doorway and the opening up of the internal panelling already described.
The 17th century first-floor window: this cross-mullioned window is currently blocked and formed part of application no. 2019/1297 for ‘Various internal works to ground, first and second floor (LBC)’ to the main house. This window is identified (no. 28) on the submitted first-floor plan (dated 18.09.2019, modified 23.02.2020) with the note: “remove existing short panel to expose the original 17c window, cover window internally with a demountable DG unit to protect original glass to window. Glass to be covered with low emissivity coating”. Recording photographically of this window is required when it is opened up. The recorder should also make notes and records as the interior panel is removed. This will form part of this contract as part of the historic building record to be included in the final report. 
N.B. It is advised that in the programme for the approved works that works to this window, and its permanent record, should be undertaken Before the courtyard extension is constructed, so as to permit the erection of suitable scaffolding, or a scaffold-tower externally to address any remedial work to the window, such as protecting the surround with pointing or mastic and the installation of any cross members to help stabilise the window from wind damage; often with lead-fixings. While this is in position the archaeologist should take the opportunity to take close-up photographs showing this window and its glazing in detail. Interior: similar records should be made of the interior face of this leaded-light window prior to, and during the fixing of the proposed secondary glazing unit, taking note of any necessary modification to be made to the interior window surround, which until the panel is removed cannot be determined. 
The plinth course since revealed, following the lowering of the external flagged floor level. Record photographs should be taken and added to the survey drawing; this was previously not visible due to an artificially raised external floor level. Detailed photographic records should be made of the complete wall showing the leaded-light window above the blocked ground-floor window, the photographs vertical to the wall face.
N.B. after the construction of the extension the roof will separate and obscure a simultaneous view of these two windows, as one will then be inside the extension; this view will be preserved in the record. 
West elevation of the Kitchen wing: the photographic and drawn record will be produced in enough detail to show the form and location of any structural features of historic significance such as blocked door-openings, masonry joints, and any other features of interest; the blocked doorway should be added to the ‘as existing’ drawings with suitable annotation and form part of the archaeological record. 
Proposed alteration: the central window of the kitchen (west side) is proposed to be removed and the walling under it opened up to provide a wide doorway (internally this is lined with brick under the windows). A new double-door will be constructed and inserted in the created opening forming a link between the new extension and the existing kitchen. It is considered - following the records already made during the stripping-out works to the interior of the kitchen - that this window is of relatively modern date and may have been inserted during the late-20th century; confirmation of this should be part of the aim of this photographic exercise.
South elevation of the additions to the kitchen: this appears to have been constructed c.1977 (archived plans dating from that era are not available). The date appears on some decorative stonework in the created patio area immediately to the west. This has three uncoordinated doorways, but with unusual decorated lintels that require recording, photographing in detail, and noting in the report; it is possible that these may have been re-used from some unknown source.
[bookmark: _Hlk44182855] Proposed alteration: the RH door will link to with the new extension (yet to be submitted for planning) and is likely to be altered, possibly widened as necessary to conform to DD and building Regs. requirements to permit wheel-chair access; however, it is not in itself of any particular merit, or original to the building. The elevation with the doorways should be carefully recorded and a note made of the small rooms that open off them (one of these was used as a dog-kennel by the previous owner. These are to be changed in the new proposal and enlarged. However, they are of recent date and of no special historic interest.
The floor area of the courtyard area should be recorded photographically showing it as it exists at the time of this survey, as best as it can, and later following the re-instatement of the original stone-flagged floor in due course – this will require a second visit and can be done when the third stage of recording is undertaken during building works (see below). 
Phase 2. The Photographic Record: A comprehensive photographic record is required of the three main external elevations of the main hall to form a permanent photographic record. However, it is likely that some of the elevations may currently be partly obscured by scaffolding. If that is the case only a couple of general shots should be taken. In due course at a later stage when all works are completed, and the scaffold has been removed, a further visit will be required to take the permanent record photographs. The fourth elevation facing south is attached on to the side of the Tudor House, this is in separate ownership. The boundary wall between the two properties should be photographed from the neighbour’s side (with permission) as this wall may have to be repaired due to cracks from instability caused by tree roots. All sides of the enclosing walled garden should also be photographed from both the outside and the inside showing its brick skin. The record of the entrance East front should also show its connection to the existing kitchen building built to the right-hand side of it, both straight-on and oblique angle shots. This will compliment the earlier Watching Brief record made of the interior of the kitchen during investigative works. A record photograph of the restored kitchen fireplace should also be taken and added to supplement the earlier record.   
Detailed photographs should first be made of the wall at the base of Darley Cliffe Hall – the plinth level where it meets the ground – and taken all the way round the building.  It is the intention of the owner and his builders  to lower the external ground-level (to form part of the Watching Brief photographic record) to prevent further and damaging damp penetration due to it being higher than the internal floor level; these photographs will help support this proposal and should be provided in advance of the completed record to assist the BMBC planning staff in evaluating this proposal. Permission for this work from the LPA will form part of a future LBC application – forthcoming, to be included in the application for a replacement extension to be built on the north side of the kitchen range that will provide a new side entrance and disabled facilities. 
The photographic record should try to give an overall impression of the size and shape of the Hall in its setting (consider using a telescopic pole) and of the kitchen ‘wing’ and its attached outbuildings on the north side. Where possible, photographs should be taken at right angles to an elevation with an appropriately sized photographic scale placed in each picture. The photographic scale should be placed in such a way as not to obscure features being recorded.
Detailed photographs should be taken of any decorative or structural detail relevant to the building’s design, development and use. Note should be made of any changes and alterations made to the historic fabric - made over time.
A photographic register should be made on site, noting the direction and subject of each photograph taken.
All photographs should be taken using a tripod mounted digital SLR with a minimum resolution of 10 mega pixels (APS-C sized sensor) and set to capture JPEG and RAW files. All RAW files will later be converted to 8-bits per channel TIFF files for the final archive.
Digital photographs must not be manipulated or altered prior to inclusion in a project archive. 
Phase 3. The Watching Brief Record:
Important note. Notification Times: Building contractors should closely liaise with the appointed buildings archaeologist, and BMBC’s Senior Conservation Officer (Tony Wiles) to ensure that they give at least 7 days prior notice of their intention to commence work. They should not begin work until the archaeologist is in attendance, except with his prior agreement. 
Monitoring. By SYAS. In addition, the works of archaeological recording may be monitored by a representative of SYAS – see para. 5.2 of the Appendix at the end of this document, section 2.2 for the required notification times to be given in advance of the commencement of works. 
Warning: Any infringement of the above requirements with works going ahead without the appointed archaeologist being in attendance may lead to criminal proceedings, and prosecution of the parties concerned by the Local Planning Authority. Such breaches of this requirement will not be tolerated.
Building works are proposed in five areas requiring the attendance of a buildings archaeologist to make records for this ‘Watching Brief’.   
1a) The courtyard extension: during opening-up of the blocked window, and its dismantling. During opening the wall through to the interior cupboard, also recording the careful storage of the stonework for re-use. During the partial dismantling of the internal wall-panelling to cut a jib door into it, and removal of the cupboard set behind the hinged panel; this should be retained for inspection. During the creation of a doorway leading through to the new extension. During the reinstatement works of transforming the window to a doorway, and the installation of the jib door and the remedial treatment of the internal passageway linking to the extension. This may involve three or four (or more) short separate visits to record work in progress and after its completion.
1b) during the removal of the kitchen window and the wall below it. 
1c) Any further excavation of the courtyard area beyond the area already dug out – following the stop notice on the advice of SYAS. 
1d) During the reinstatement of the stone flagged floor and showing it on completion.
1e) A copy of the short report on the building work done to the courtyard area, made by Paul Furniss, should be provided by the client to the appointed contractor to provide background for this present recording brief. However, this should not form part of the archaeological record, though it may be briefly referred to in the final report and a separate copy included within the project archive for local deposition and to the HER at SYAS.
2. The main house external plinth: excavation and lowering of the ground-level around the main house. This may be a lengthy process, but only periodic records need be made to ensure records are made both before, during, and after these works, but before any further remedial measures.
3. The attic bathroom rooflight. During the creation of a hole in the roof and cutting through the rafters to permit the installation of a fire-escape rooflight as shown on the second floor plan of application no. 2019/1297 Note no. 38 ‘Install new conservation roof light to bathroom’. See 2nd floor plan:
https://wwwapplications.barnsley.gov.uk/PlanningExplorerMVC/Home/ApplicationDetails?planningApplicationNumber=2019%2F1297
4. The proposed replacement extension: attached to the north gable of the kitchen – yet to be submitted for planning approval. 
5. The boundary wall between Tudor House and Darley Cliffe
The recent extension (3a) will require the attendance of the buildings archaeologist during the later stages of the demolition of the present building. This is not considered of any historic interest having only been constructed during the last 30 or so years from reclaimed stonework. Also for any ground disturbance - for clearance and excavation and trenching for new foundations and drainage. Map evidence highlights the possibility of earlier building foundations being revealed during this work. Drawn and photographic records as appropriate should be made in accordance with any on-site instructions issued by the BMBC staff or SYAS or the clients historic buildings consultant. 
Written record 
Site-notes should be made during all of the above works, in addition to the photographic and drawn record. This is to aid the preparation of short individual reports for each of the three stages of development as described above. This is to aid both the client and contractor so that each completed stage can be billed as the programme of work progresses that may take several months.
	Reporting 
Following the completion of the reports these will then be summarised in a final report into the findings of the various stages of recording. This will be sent to the BMBC’s CO within a maximum timescale of eight weeks on completion of all fieldwork, unless otherwise agreed.  
The final report should include an introduction and an executive summary into the findings of the recording. This report should also include the results of any historical research undertaken and include copies of the historic sequence of O.S. maps, a description of each feature recorded, and a discussion and conclusion into the findings referencing the three separate reports as necessary that should be included within the final report folio. 
This final report should have a clear and distinct purpose, avoiding unnecessary repetition. Any discussion or conclusion sections should do more than simply reproduce elements of the site narrative.
The report should include a full bibliography (if relevant), a quantified index to the site archive, and a copy of this specification as an appendix. All final versions of the written report must include a copy of the relevant Online Access to the Index of archaeological investigations (OASIS) data collection form.
The information content of the written report will become publicly accessible once deposited with BMBC, unless confidentiality is explicitly requested, in which case it will become publicly accessible six months after deposit.  
The material presented within the report may be used by the BMBC, and any deposit with the regional HER will be in perpetuity, although the historic environment contractor retains the right to be identified as the author, or creator of any parts of the document as specified in the Copyright, Designs and Patents Act 1988 (Chapter IV, Section 79).  The permission will allow the LPA (BMBC) to reproduce material, including for non-commercial use by third parties, with the copyright owner suitably acknowledged.
Report Illustrations should include:
A location map at a scale sufficient to allow clear identification of DC in relation to other buildings in its immediate curtilage. 
· Any relevant historic photographs or map editions, with the position of the DC and the Kitchen wing and courtyard clearly indicated.
· A complete set of site drawings to Historic England standards (to include a ground-floor plan, external and internal elevations where relevant – such as in the Dining room. 
· An annotated set of plans of the building recorded, on which the position and direction of each photographic shot is marked.
When captioning photographs, these should identify the individual photographs by means of a running sequence of numbers (e.g. Plate no. 1; Plate no. 2), and it is this numbering system which should be used in cross-referencing throughout the report and on the photographic plans. However, the relevant original digital frame (if relevant) should be included in brackets at the end of each caption. A maximum of two plates per side of A4 will be sufficient for the final report
Health and Safety 
Contractors are expected to abide by the 1974 Health and Safety at Work Act and its subsequent amendments. Where archaeological work is carried out at the same time as the work of other contractors, regard should be taken of any reasonable additional constraints that these contractors may impose. Appropriate provision of first aid, telephone and PPE should be followed.
The safety of the individual will not be compromised in any way for the sake of the record.
Insurance
It is the contractor’s responsibility to ensure that they have adequate public and professional insurance cover.
The Archive
The final stage of the project is the submission of a project archive to an appropriate repository following the requirements of BMBC’s Conservation Officer. A project is not considered complete until the archive has been deposited and the final report is publicly accessible.
An OASIS form will be completed and a digital copy of the report uploaded to the OASIS website. Following deposit with the SYAS Historic Environment Record it will be made available as grey literature by the Archaeology Data Service (ADS) and a full digital archive shall be created and deposited with the them and copy to BMBC Planning Department.  
All material originally created in a digital form must be prepared for deposition according to recognised standards and guidelines such as those made available by the Archaeology Data Service (http://guides.archaeologydataservice.ac.uk/). 
The archive should consist of all records created during the project (both hard copy and digital). Archives should be prepared to relevant minimum standards and adhered to the guidelines set by the Chartered Institute of Archaeologists (CIfA, 2014b),). Digital file names need to meet the requirements of the South Yorkshire County Record Office (https://www.syas.gov.uk/record-office-policies-and-deposits) and produced in line with guidance set out in Digital Image Capture and File Storage (Historic England, 2016b).
Archives should be submitted to the agreed repository within 150 working days of the submission of a project’s final written report.

Peter Thornborrow, 30.06.2020

Sources consulted
Archaeology Data Service 2018: Guide to Good Practise (available at: http://guides.archaeologydataservice.ac.uk/)
CIfA 2014a: Chartered Institute for Archaeologists Standard and guidance for the archaeological investigation and recording of standing buildings or structures (available at http://www.archaeologists.net/sites/default/files/CIfAS&GBuildings_1.pdf) 
CIfa 2014b: Standard and guidance for the creation, compilation, transfer and deposition of archaeological archives (available at https://www.archaeologists.net/sites/default/files/CIFAS&GArchives_2.pdf ) 
Historic England 2016a: Understanding Historic Buildings: A Guide to Good Recording Practice (available at https://historicengland.org.uk/images-books/publications/understanding-historic-buildings/heag099-understanding-historic-buildings/)
Historic England 2016b: Digital Image Capture and File Storage: Guidelines for Best Practice (available at https://historicengland.org.uk/images-books/publications/digital-image-capture-and-file-storage/)


Appendix
0.1 Draft conditions prepared by BMBC for Courtyard extension: Darley Cliffe Hall, March 2020 

1. The development hereby permitted shall be begun before the expiration of 3 years from the date of this permission.
Reason:  In order to comply with the provision of Section 91 of the Town and Country Planning Act 1990. 

1. The development hereby approved shall be carried out strictly in accordance with the amended plans (Nos.) and specifications as approved unless required by any other conditions in this permission.
Reason: In the interests of the visual amenities of the locality in accordance with Local Plan Policy D1 High Quality Design and Place Making.

1. No development, including any demolition and groundworks, shall take place until the applicant, or their agent or successor in title, has submitted a Written Scheme of Investigation (WSI) that sets out a strategy for archaeological investigation and this has been approved in writing by the Local Planning Authority.
 
1. The WSI shall include: 

The programme and method of site investigation and recording.
The requirement to seek preservation in situ of identified features of importance.
The programme for post-investigation assessment. 
The provision to be made for analysis and reporting. The provision to be made for publication and dissemination of the results. 
The provision to be made for deposition of the archive created. 
Nomination of a competent person/persons or organisation to undertake the works.
The timetable for completion of all site investigation and post-investigation works.
Thereafter the development shall only take place in accordance with the approved WSI and the development shall not be brought into use until the Local Planning Authority has confirmed in writing that the requirements of the WSI have been fulfilled or alternative timescales agreed. 

Reason: To ensure that any archaeological remains present, whether buried or part of a standing building, are investigated and a proper understanding of their nature, date, extent and significance gained, before those remains are damaged or destroyed and that knowledge gained is then disseminated. 

5.2	 On commencement of the works, a representative sample of all external materials shall be provided and approved in writing by, the Local Planning Authority, and the development shall proceed in strict accordance with these details as approved. 

Reason: In the interests of the visual amenities of the locality and in accordance with Local Plan Policy HE3 Developments affecting Historic Buildings and D1 High Quality Design and Place Making
5.3  I would also appreciate it if you could confirm the plan references 
5177-PBA-ZZ-GF-DR-A(00)04-A1-P.01 received 24th February 2020
Design and Access Statement
Heritage Statement
Addendum to Design and Access Statement and Heritage Statement received 25th February 2020




0.2 MODEL BRIEF FOR ARCHAEOLOGICAL MONITORING (WATCHING BRIEF) prepared by the South Yorkshire Archaeology Service (SYAS) Supplied by Andrew Lines
1  SUMMARY 
1.1  There is reason to believe that archaeological remains may be disturbed in the course of the proposed development, though little is known of their character, extent and state of preservation. 
 1.2  Where provided, an accompanying planning report outlines the known or suspected archaeological implications of development on the development site. 
 1.3  Archaeological monitoring (often referred to as a ‘Watching Brief’) is required to ensure that remains that are to be affected by works will be recorded and/or retrieved. 
1.4  All archaeological work will comply with:
  “Regional statement of good practice for archaeology in the development process, Yorkshire, the Humber & the North East” (available for download from the SYAS website);
  relevant IfA Standard and Guidance documents; 
 relevant EH best practice guidance documents. 
 1.5  All archaeological work will be monitored by the South Yorkshire Archaeology Service (SYAS). 

 2  FIELDWORK METHODOLOGY 
2.1  The work will be carried out by appropriately qualified and experienced staff,.  Details of staff numbers, their roles and relevant experience will be provided to SYAS.  Staff CVs will be submitted (unless already supplied to SYAS in previous project specifications).  Any sub-contracted specialists will be subject to the same provisions. 
 2.2  NOTIFICATION OF COMMENCMENT OF WORK: 
Reasonable prior notice (at least 14 days) of the commencement of the development is to be given to the archaeological contractor.  A minimum of one week’s notice of the commencement of fieldwork must be given by the archaeological contractor to SYAS, to arrange monitoring visits. 
 2.3  Access to the site must be afforded to the developer's nominated archaeological contractor at all reasonable times. 
 2.4  All groundworks, including those associated with the construction of foundations and service trenches, must be undertaken under archaeological supervision, to allow for the identification and recording of any archaeological material that might be uncovered.  
2.5  Where structures, features or finds of potential archaeological interest are exposed or disturbed by construction works, sufficient time will be allowed for the archaeological contractor to clean, assess and, where appropriate, hand excavate, sample and record these features and finds. 
2.6  All record photographs will be on black and white film and 35mm colour slide film. 
 2.7  Digital photography can only be used to supplement the photographic record; it must not form any part of the primary archive. 
 2.8  Any human remains that are revealed must initially be left in situ and, if removal is necessary, this must comply with the relevant Ministry of Justice (formerly Home Office), Diocesan and other regulations, as appropriate. 
 2.9  All finds that are ‘treasure’ (in terms of the Treasure Act 1996) will be reported to the Coroner and appropriate procedures then followed. 
 2.10  Heavy plant or excavators must not be operated in the immediate vicinity of archaeological remains until the remains have been recorded and the archaeological contractor on site has given explicit permission for operations to recommence at that location. 
 2.11  Where archaeological remains are observed or suspected by contractors or plant operators, they must immediately cease work and notify the archaeological contractor. 
 2.12  If it becomes clear during the monitoring that little of archaeological interest is likely to survive on the site, the contractor should discuss their work with SYAS.  A joint decision will then be made on reducing the work to an intermittent watching brief or ceasing observation of groundworks. 

 3  POST-EXCAVATION GUIDELINES 
3.1  For all categories of material recovered, including finds, palaeo-environmental, industrial and other specialist samples, an assessment by an appropriately experienced specialist will be undertaken.  Samples must be processed and sorted, and any artefacts recovered provided to the appropriate specialist(s) to be considered alongside the hand-recovered material.  Basic stratigraphic information will be supplied to the project specialists. 
 3.2  All finds are to be treated in accordance with current EH best practice, including 'Investigative Conservation'.  Finds are to be cleaned and marked according to accepted principles and in line with appropriate period/ material guidelines. 
 3.3  The site archive will be prepared in accordance with the UKIC’s document Guidelines for the Preparation of Excavation Archives for Long Term Storage and the IfA’s “Standard And Guidance for the creation, compilation, transfer and deposition of archaeological archives”. 


 4  REPORTING 
4.1  The monitoring will result in a report including background information (with planning application details, where appropriate), methods, detailed results, discussion and conclusions. 
 4.2  Illustrations to be included are:  
 a detailed location map.  
 a detailed site plan, as excavated. 
 detailed plans of relevant features, as excavated. 
 detailed sections of relevant features, as excavated.
 an overall site plan showing all (phased) archaeological features recorded. 
 selection of photographs of work in progress. 
 select artefact illustrations and/or photographs. 
 4.3  The results of assessment/analysis of all find categories, by appropriate specialists, will be included in the report. 
 4.4  The results of assessment/analysis of palaeo-environmental, industrial and other samples, by appropriate specialists, will be included in the report. 
4.5  The results of any scientific dating undertaken will be included in the report. 
 4.6  The report will include a phased interpretation of the site, if possible, and consider the results in their local and regional context. 
4.7  The report will include a detailed context index and an index to the archive. 
 4.8  A printed and bound copy of the report must be supplied to SYAS for incorporation into the South Yorkshire Sites and Monuments Record.  A digital copy of the report must also be supplied to SYAS and to the EH Science Advisor. 
 4.9  A summary report of an appropriate length, accompanied by illustrations (at 300dpi resolution), must be prepared and submitted in digital format, for publication in the appropriate volume of Archaeology in South Yorkshire. 
 4.10  Provision will be made for publicising the results of the work locally, e.g. by presenting a paper at South Yorkshire Archaeology Day and talking to local societies. 
 4.11  The archaeological contractor must complete the online OASIS form at http://ads.ahds.ac.uk/project/oasis/. 
4.12  A contingency will be made for the preparation and publication, in a local, regional or national journal, of the results of the monitoring. 


 5  DEPOSITION OF ARCHIVE AND FINDS 
5.1  Arrangements for the deposition of the finds and site archive will be made with the relevant museum service in advance of commencement of fieldwork.  The relevant service can be found via the ‘Archaeological Collections Areas Database and Map’ on the ADS website.   
 5.2  “Archaeological Archive Deposition Policy for Museums in Yorkshire and the Humber” created a uniform region-wide approach to the preparation and deposition of archaeological archives.  The resulting formal process requires the completion and submission of forms to the relevant museum service at the project initiation, mid-point review and completion stages (template forms are available for download from the SYAS website). 
5.3  The archaeological contractor will contact the museum’s archaeological curator or collections manager to discuss archaeological archiving requirements at the initial stage of preparation of the project design.  Following agreement with the client, details of archiving arrangements will be incorporated into the project design.  This will include confirmation that a budget to cover the museum’s deposition charge has been allowed for. 
 5.4  The museum services do not accept digital archives; digital archiving will need to be discussed with ADS (or equivalent service) and appropriate costs allowed for. 
 5.5  Archiving is expected to be carried out as specified, in a timely manner.  On completion, confirmation of deposition will be supplied to SYAS. 
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