[bookmark: _GoBack]23 King Street Proposed front elevation
Stone pillar and scroll above to be exposed, cleaned made good.
Sign (details provided)
Stone plinth to be cleaned, repointed and made good.
White uPVC windows and door to remain
Rainwater pipe Black
Painted stone front elevation at first floor. To be repainted in stone to blend in with natural colour of existing stone.
Timber cornice. Lead flashing to be restored. Painted to match sign background colour.
Stone cills, lintels and window surround feature to be painted in stone colour 
Terracotta tiled roof
Brick chimney
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