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	Measures to prevent mud and debris
on the highway


Project: Detached dwelling
Site address:
Land to the rear of 11 &13 Hillside Crescent
Brierley
Barnsley
[bookmark: h.1kmozguib79q]Description of activity
During construction all site traffic, workmen and deliveries will remain on the existing tarmac hardstanding.
Deliveries will have a dedicated banksman in appropriate hi-vis and personal protective equipment to guide them in manoeuvring around the hardstanding and prevent them going off road.
Any plant which must leave the hardstanding, eg during foundation dig, will be cleaned using the on-site pressure washer, to ensure no mud is dragged onto the highway.
During the working day it will be the site manager's responsibility to check the highway, in the morning and afternoon, and be prepared to call for a road sweeper if any contamination has occurred.
[bookmark: h.ygmyk6vg3h9j]Supervision
· MR F Ayres or his appointed Site Supervisor
[bookmark: h.ocmnip9mxfv8][bookmark: h.r46xzs9m3ioz]Legislation
· Health and Safety Work Act 1974
· The Management of Health and Safety at Work Regulations 2006
· Workplace (Health, Safety and Welfare) Regulations 1992
· The Control of Asbestos Regulations 2012
· Provision and Use of Work Equipment Regulations (PUWER) 1998
· Control of Substances Hazardous to Health Regulations 2002
· The Work at Height Regulations 2005
· The Personal Protective Equipment at Work Regulations 2002
· The Manual Handling Operations Regulations 1992
· The Construction (Design and Management) Regulations 2015
· Electricity at Work Regulations 1989
· The Pressure Systems Safety Regulations 2000
· Pressure Equipment Regulations 1999 (SI 1999/2001)
[bookmark: h.2cpfsm4rqcx7][bookmark: h.ddte95cmjn8g]PPE requirements
· Hard hats
· Safety boots
· Hi-vis vest
· Safety gloves
· Safety glasses
[bookmark: h.jjom1h6ke549][bookmark: h.zai7l19dxpwv]First aid
Refer to the onsite safety notice board for all first aid information. 

A first aid box with enough equipment to cope with the number of workers on site should be provided for by the client or principal contractor. 

The client or principal contractor should nominate an appointed person to take care of first-aid arrangements. 

The number of appointed first aiders shall be dependent on the number of employees.
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