[bookmark: page1] [image: ]CONSTRUCTION METHOD STATEMENT

2017/1609/FUL | RESIDENTIAL DEVELOPMENT FOR SIX NEW SEMI DETACHED DWELLINGS.
[image: ]
1. INTRODUCTION


This Construction Method Statement (CMS) is prepared by Jrb Designs Ltd. The statement lists the construction method of 6 no. new  semi detached dwellings on land at Laxton Road, Athersley North, Barnsley, South Yorkshire, S71 3DH. The CMS is required by planning condition 4 attached to planning permission reference 2017/1609/FUL. Condition 4 sets out the requirements of the CMS. This CMS document is intended to enable discharge of condition 4.
This CMS sets out proposed measures to minimize and mitigate construction impact on the highways during the construction phase. Consideration is in accordance with Policy D14 of the Council's Local Development Framework, Development Policies Document. It is intended that the CMS remains under review during the construction of the project. Further details of the construction programme can be provided if required.




1. THE PARKING OF SITE OPERATIVES AND VISITOR’S VEHICLES


[bookmark: _GoBack]Parking of onsite operative’s vehicles will be kept to a minimum throughout the duration of the build. Parking will be considerate of all neighbours. There will be 4 onsite parking spaces indicated as Area C in Site layout. The total onsite parking area measures 6m x 11m. 3 road side spaces are available should further parking be required (Indicated in Figure 1, Area E). The site manager will ensure that the road side parking does not inhibit pedestrians or cause congestion within the vicinity of the site. Due to the small scale of the build we will ensure that onsite operatives are kept to a minimum and advise site operatives to car share or use sustainable modes of transport where possible.



2. LOADING AND UNLOADING OF PLANT AND MATERIALS


Construction materials will be unloaded at the site entrance. Indicated as Area A in Figure 1. This area is approximately 9m x 5m Due to the size of the frontage of the plot a banksman
























[bookmark: page3] [image: ]will ensure all materials are unloaded from the road side onto the unloading area. We will ensure that deliveries are dropped in planned timely slots to avoid any congestion on the roads nearby and all deliveries will be within reasonable hours to mitigate any negative impacts to neighbouring properties.




3.MANAGEMENT OF CONSTRUCTION TRAFFIC AND ACCESS ROUTES


Construction traffic have access to the site from Barnsley via the A61  which enters Athersley North Then turn right onto Newstead Road at the roundabout turn right onto Lindhurst Road then left onto Laxton Road. 




4. STORAGE OF PLANT AND MATERIALS USED IN CONSTRUCTING
THE DEVELOPMENT


The unloading area shown in Site layout, will be a temporary storage area and all materials will be transferred to Area B (Site layout). A 2.4m x 2.4m secure container will be placed to the frontage of the construction area, shown in Figure 1 as Area D where smaller items will be securely stored. This will be removed once the build is complete.
Large scale items will be stored in the temporary storage area unless they can be safely moved to Area B. Throughout the construction phase we will plan for large items to be delivered as close as possible to the correct stage of the build so that they are not laid around the site. These will be dealt with as part of our Health and Safety program for the build. The largest item expected on the site will be roofing rafters and floor joists these will be moved to area B for safety purposes. Site security fencing will be erected to the frontage of the site as well as security cameras.
[bookmark: page4] [image: ]5.WHEEL WASHING FACILITIES


Prevention of Mud and Debris leaving site The intended parking area within the site will be temporarily surfaced with MOT type I. Wheel cleaning will be provided where necessary to avoid debris on the highway. In addition to this we will engage Road Sweeping Services to make a pass for the extent of the affected highway along Laxton Road. This will be available on standby and to be called out as and when required.
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