JRB DESIGNS Ltd.

1 SAVILLE STREET,

CUDWORTH,

BARNSLEY,

SOUTH YORKSHIRE,

S72 8LT.

Registration No. 3372719

TEL. 01226 383542

MOB. 07970541192
e-mail john@jrbdesigns.co.uk
Sustainable Drainage report for the development of 14 new dwellings off Acorn Way Grimethorpe Barnsley.
 The purpose of this report is to assess the potential for disposing of surface water through a sustainable drainage system (SuDS) to satisfy a planning application for 12 new dwellings at the site address (the Site). The site on Acorn Way Grimethorpe lies in an urban area which is neither at risk of flooding from rivers or surface water.
At present the site is covered by 70% non permeable surface consisting of a large tarmac area and is flat. The proposal will actually reduce the non permeable surface area to 40%. This is achieved by replacing the existing tarmac hard standing with permeable block paving. It is also proposed that the roof surface water be channelled into a  soak away to the rear of the buildings. The relatively high permeability of the Sandstone Formation may create potential for a soak away SuDS feature in all areas of the Site. However, the permeability of the ground here will have to be investigated by way of percolation testing to verify the feasibility of such a scheme. 
Maximum groundwater levels should be sufficiently below the base of potential infiltration soak aways. 
