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Project: 
Minor alterations to 24 High Street, Goldthorpe, Barnsley, S63 9LR

Preliminary
This document is submitted as a supporting document for alterations to the above which are summarised below.

1.0	Summary of Alterations

1.1 The following alterations are proposed in the submitted planning application

1.1.1 Side elevation window retained but glazing replaced with obscure glazing. Window altered to be bottom hung for natural ventilation purposes with window fitted with a restrictor to prevent it opening onto the pavement and providing a hazard. The restrictor is to remain in place for the life of the use.
1.1.2 Existing rear access door to be blocked up in like for like materials to that adjacent.
1.1.3 Existing rear window to be converted to a door by breaking out the masonry below the window. This door is to be 30 minute fire rated.
1.1.4 Ramp to be formed externally to 1.1.3 to provide accessible entry into the building.
1.1.5 Front elevation first floor window to be altered to provide an escape window. Materials to match existing.
1.1.6 Existing rear window to be converted to provide access to first floor (existing internal stair to be removed).
1.1.7 Metal access stair to be provided to rear to provide access to first floor level.
1.1.8 Ground floor use to remain in Planning Use Class E.
1.1.9 First floor to be converted to domestic use. 

1.2	Design and Access Statement

1.2.1	Very minor alterations are proposed as part of this application, following is a brief commentary on design and access.

1.2.2	Minor elements of the existing building have been altered, mostly in areas that have zero impact on the design. The revision to GFL access and alteration to front window at FFL are minor and in keeping with the street scene, which has an abundance of different window styles. The metal access stair to the rear matches similar staircases on adjacent properties and has been designed to match those staircases.

1.2.3	Access into the building is retained as existing on the front elevation (accessible type stair) and has been improved at the rear to allow wheelchair accessibility for staff or visitors.

1.2.4	No other elements of design or access have been altered in this scheme.
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