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Metropolitan Borough Council




	To: 
	Development Management
Fao Keith Pell


	My Ref: 2016/0051

	
	Your Ref:  
	

	Date: 19/02/2016
	
	Tel:
	B Wilson
	Ext:
	2177


Burton Road, Monk Bretton
Dwelling

Reference is made to the above application.
There are no objections in principle to the proposed development in a highway context, subject to the following conditions being included in any subsequent planning consent:-
1. The parking/manoeuvring facilities, indicated on the submitted plan, shall be surfaced in a solid bound material ( ie not loose chippings) and made available for the manoeuvring and parking of motor vehicles prior to the development being brought into use, and shall be retained for that sole purpose at all times.

Reason: to ensure that satisfactory off street parking/manoeuvring are provided, in the interests of highway safety and the free and safe flow of traffic and in accordance with Core Strategy Policy CSP26, New Development and Highway Improvement.

2. Pedestrian intervisibility splays, having the dimensions 2m x 2m, shall be safeguarded at the drive entrance/exit such that there is no obstruction to visibility at a height exceeding 600mm above the nearside channel level of the adjacent highway, in the interest of road safety.
3. Vehicular and pedestrian gradients within the site shall not exceed 1:12 to ensure safe and adequate access.

For and on behalf of 

Head of Highways, Engineering & Transportation

Place





Environment & Transport
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